{"text_format":"3","workbook":"xlsx","n_sheets":7,"sheets":["main","cars","chassis","engine","tranny","turbos","sources"],"not_rendered":{"macros":1,"defined_names":6},"read":"whole","date_system":"1900"}

{"sheet":"main","index":0,"n_rows":42,"n_cols":15,"rows_kept":42}
[]
["Volvo Database Spreadsheet"]
[]
["The sheet 'cars' lists data for Volvo models.  That sheet lists the main components (chassis, engines, etc) by specific names."]
["Component details are supplied by the other sheets."]
["If you are adding or correcting data, please highlight your changes so that I can more easily incorporate the revisions."]
[]
["- Bill Garland <garlandw@mcmaster.ca>"]
["-www.nuceng.ca/bill/volvo/volvohome.htm"]
[]
[]
[]
[]
[]
["Macros to generate html files"]
["(for webmaster use only)"]
{"$rows_empty":7}
["Volvo database (for illustration only - the actual data is entered directly into the subsequent sheets, not here)"]
[]
["Structure of database"]
[]
["car","name","year","chassis 0","chassis 1","chassis 2","engine","turbo","tranny 0","diff","tranny 1","diff","tranny 2","diff","notes"]
[]
["chassis","name","family","#doors","wb","len","width","height","wt","turn rad","front suspension","rear suspension","notes"]
[0]
[1]
[2]
["engine","name "," #cyl "," #valves "," disp ","compression "," fuel type "," fuel delivery "," turbo "," Notes"]
[]
["tranny","name "," type "," maker "," #gears "," r1 "," r2 "," r3 "," r4 "," r5 "," r6 "," r7 "," Notes"]
[0]
[1]
[2]
["turbo","Turbo name","Notes"]
[]
["sources","Source ID","Notes"]

{"sheet":"cars","index":1,"n_rows":866,"n_cols":14,"rows_kept":866}
["Volvo Car Page",null,"as of Dec 8, 2011"]
[{"$f":"COUNTA(A4:A1092)","v":863}]
["name","year","chassis 0","chassis 1","chassis 2","engine","turbo","tranny 0","diff","tranny 1","diff2","tranny 2","diff3","notes"]
["OV4",1927,"OV4open","OV4pickup","OV4frame","DA",null,"manual",0,null,0,null,0,"'Öppen Vagn' or Open top, 28 HP, the pickup version was called the OV4 TV.[LINDH]"]
["PV4",1927,"PV4sedan","PV4frame",null,"DA",null,"manual",0,null,0,null,0,"Person Vagn, 28 HP. [LINDH]"]
["OV4",1928,"OV4open","OV4pickup","OV4frame","DA",null,"manual",0,null,0,null,0,"'Öppen Vagn' or Open top, 28 HP, the pickup version was called the OV4 TV. [LINDH]"]
["PV4",1928,"PV4sedan","PV4frame",null,"DA",null,"manual",0,null,0,null,0,"Person Vagn, 28 HP. [LINDH]"]
["OV4",1929,"OV4open","OV4pickup","OV4frame","DA",null,"manual",0,null,0,null,0,"'Öppen Vagn' or Open top, the pickup version was called the OV4 TV"]
["PV4",1929,"PV4sedan","PV4frame",null,"DA",null,"manual",0,null,0,null,0,"Person Vagn, 28 HP. [LINDH]"]
["PV650",1929,"PV650frame",null,null,"DB",null,"manual",0,null,0,null,0,"Frame only, 55 HP. [LINDH]"]
["PV651",1929,"PV651sedan",null,null,"DB",null,"manual",0,null,0,null,0,"55 HP. [LINDH]"]
["PV652",1929,"PV652sedan",null,null,"DB",null,"manual",0,null,0,null,0,"55 HP, trim level differences from the PV651. [LINDH]"]
["PV650",1930,"PV650frame",null,null,"DB",null,"manual",0,null,0,null,0,"Frame only, 55 HP. [LINDH]"]
["PV651",1930,"PV651sedan",null,null,"DB",null,"manual",0,null,0,null,0,"55 HP. [LINDH]"]
["PV652",1930,"PV652sedan",null,null,"DB",null,"manual",0,null,0,null,0,"55 HP, trim level differences from the PV651. [LINDH]"]
["TR670",1930,"TR670frame",null,null,"DB",null,"manual",0,null,0,null,0,"Taxi, frame only, 55 HP. [LINDH]"]
["TR671",1930,"TR671taxi",null,null,"DB",null,"manual",0,null,0,null,0,"Also known as the TRS.  Taxi body with partition, extra headroom and fixed front seats, urban use, 55 HP. [LINDH]"]
["TR672",1930,"TR671taxi",null,null,"DB",null,"manual",0,null,0,null,0,"Also known as the TRL.  Taxi body without partition and movable front seats, rural use, 55 HP. [LINDH]"]
["PV650",1931,"PV650frame","PV650special",null,"DB",null,"manual",0,null,0,null,0,"Frame only, 55 HP. [LINDH]"]
["PV652",1931,"PV652sedan",null,null,"DB",null,"manual",0,null,0,null,0,"55 HP, trim level differences from the PV651. [LINDH]"]
["TR670",1931,"TR670frame",null,null,"DB",null,"manual",0,null,0,null,0,"Taxi, frame only, 55 HP. [LINDH]"]
["TR671",1931,"TR671taxi",null,null,"DB",null,"manual",0,null,0,null,0,"Also known as the TRS.  Taxi body with partition, extra headroom and fixed front seats, urban use, 55 HP. [LINDH]"]
["TR672",1931,"TR671taxi",null,null,"DB",null,"manual",0,null,0,null,0,"Also known as the TRL. Taxi body without partition and movable front seats, rural use, 55 HP. [LINDH]"]
["TR673",1931,"TR671taxi",null,null,"DB",null,"manual",0,null,0,null,0,"Taxi body with partition, extra headroom and fixed front seats, urban use, wider and longer than the TR671, 55 HP. [LINDH]"]
["TR674",1931,"TR671taxi",null,null,"DB",null,"manual",0,null,0,null,0,"Taxi body without partition and movable front seats, rural use, wider and longer than the TR672, 55 HP. [LINDH]"]
["PV650",1932,"PV650frame","PV650special",null,"DB",null,"manual",0,null,0,null,0,"Frame only, 55 HP. [LINDH]"]
["PV652",1932,"PV652sedan",null,null,"DB",null,"manual",0,null,0,null,0,"55 HP, trim level differences from the PV651. [LINDH]"]
["TR670",1932,"TR670frame",null,null,"DB",null,"manual",0,null,0,null,0,"Taxi, frame only, 55 HP. [LINDH]"]
["TR673",1932,"TR671taxi",null,null,"DB",null,"manual",0,null,0,null,0,"Taxi body with partition, extra headroom and fixed front seats, urban use, wider and longer than the TR671, 55 HP. [LINDH]"]
["TR674",1932,"TR671taxi",null,null,"DB",null,"manual",0,null,0,null,0,"Taxi body without partition and movable front seats, rural use, wider and longer than the TR672, 55 HP. [LINDH]"]
["PV650",1933,"PV650frame","PV650special",null,"DB",null,"manual",0,null,0,null,0,"Frame only, 55 HP. [LINDH]"]
["PV652",1933,"PV652sedan",null,null,"DB",null,"manual",0,null,0,null,0,"55 HP, trim level differences from the PV651. [LINDH]"]
["PV653",1933,"PV653sedan",null,null,"EB",null,"manual",0,null,0,null,0,"65 HP, base model.  Based on the PV652 but with an all-metal body. [LINDH]"]
["PV654",1933,"PV653sedan",null,null,"EB",null,"manual",0,null,0,null,0,"65 HP, deluxe trim model.  Based on the PV652 but with an all-metal body. [LINDH]"]
["PV655",1933,"PV655frame",null,null,"EB",null,"manual",0,null,0,null,0,"65 HP, frame only. [LINDH]"]
["TR670",1933,"TR670frame",null,null,"DB",null,"manual",0,null,0,null,0,"Taxi, frame only, 55 HP. [LINDH]"]
["TR673",1933,"TR671taxi",null,null,"DB",null,"manual",0,null,0,null,0,"Taxi body with partition, extra headroom and fixed front seats, urban use, wider and longer than the TR671, 55 HP. [LINDH]"]
["TR674",1933,"TR671taxi",null,null,"DB",null,"manual",0,null,0,null,0,"Taxi body without partition and movable front seats, rural use, wider and longer than the TR672, 55 HP. [LINDH]"]
["PV650",1934,"PV650frame","PV650special",null,"DB",null,"manual",0,null,0,null,0,"Frame only, 55 HP. [LINDH]"]
["PV653",1934,"PV653sedan",null,null,"EB",null,"manual",0,null,0,null,0,"65 HP, base model.  Based on the PV652 but with an all=metal body. [LINDH]"]
["PV654",1934,"PV653sedan",null,null,"EB",null,"manual",0,null,0,null,0,"65 HP, deluxe trim model.  Based on the PV652 but with an all-metal body. [LINDH]"]
["PV655",1934,"PV655frame",null,null,"EB",null,"manual",0,null,0,null,0,"65 HP, frame only. [LINDH]"]
["TR670",1934,"TR670frame",null,null,"DB",null,"manual",0,null,0,null,0,"Taxi, frame only, 55 HP. [LINDH]"]
["TR673",1934,"TR671taxi",null,null,"DB",null,"manual",0,null,0,null,0,"Taxi body with partition, extra headroom and fixed front seats, urban use, wider and longer than the TR671, 55 HP. [LINDH]"]
["TR674",1934,"TR671taxi",null,null,"DB",null,"manual",0,null,0,null,0,"Taxi body without partition and movable front seats, rural use, wider and longer than the TR672, 55 HP. [LINDH]"]
["TR675",1934,"TR670frame",null,null,"EB",null,"manual",0,null,0,null,0,"Taxi, frame only, 70 HP. [LINDH]"]
["TR676",1934,"TR671taxi",null,null,"EB",null,"manual",0,null,0,null,0,"Taxi body with partition, extra headroom, urban use, 70 HP. [LINDH]"]
["TR677",1934,"TR677frame",null,null,"EB",null,"manual",0,null,0,null,0,"Taxi, frame only, 70 HP. [LINDH]"]
["TR678",1934,"TR678taxi",null,null,"EB",null,"manual",0,null,0,null,0,"Taxi, rural use, with partition, lower roof, 70 HP. [LINDH]"]
["TR679",1934,"TR678taxi",null,null,"EB",null,"manual",0,null,0,null,0,"Taxi, rural use, without partition, lower roof, 70 HP. [LINDH]"]
["PV36",1935,"PV36sedan",null,null,"EC",null,"manual",0,null,0,null,0,"84 HP, new 'American-like' sleek steel body on frame. One convertible made. [LINDH]"]
["PV655",1935,"PV655frame",null,null,"EB",null,"manual",0,null,0,null,0,"65 HP, frame only. [LINDH]"]
["PV656",1935,"PV656frame",null,null,"EC",null,"manual",0,null,0,null,0,"80 HP, frame only. [LINDH]"]
["PV657",1935,"PV657frame",null,null,"EC",null,"manual",0,null,0,null,0,"80 HP, frame only for ambulances. [LINDH]"]
["PV658",1935,"PV658sedan",null,null,"EC",null,"manual",0,null,0,null,0,"80 HP, base version. [LINDH]"]
["PV659",1935,"PV658sedan",null,null,"EC",null,"manual",0,null,0,null,0,"80 HP, deluxe version. [LINDH]"]
["TR676",1935,"TR671taxi",null,null,"EB",null,"manual",0,null,0,null,0,"Taxi body with partition, extra headroom, urban use, 70 HP. [LINDH]"]
["TR678",1935,"TR678taxi",null,null,"EB",null,"manual",0,null,0,null,0,"Taxi, rural use, with partition, lower roof, 70 HP. [LINDH]"]
["TR701",1935,"TR671taxi",null,null,"EC",null,"manual",0,null,0,null,0,"Taxi, with partition, 80 HP. [LINDH]"]
["TR702",1935,"TR677frame",null,null,"EC",null,"manual",0,null,0,null,0,"Taxi, frame only, 80 HP. [LINDH]"]
["TR703",1935,"TR678taxi",null,null,"EC",null,"manual",0,null,0,null,0,"Taxi, with partition, 80 HP. [LINDH]"]
["TR704",1935,"TR678taxi",null,null,"EC",null,"manual",0,null,0,null,0,"Taxi, without partition, 80 HP. [LINDH]"]
["PV36",1936,"PV36sedan",null,null,"EC",null,"manual",0,null,0,null,0,"84 HP, new 'American-like' sleek steel body on frame. [LINDH]"]
["PV51",1936,"PV51sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Base version. 86 HP, steel body on frame. [LINDH]"]
["PV51ch/V51ch",1936,"PV51frame",null,null,"EC",null,"manual",0,null,0,null,0,"'Frame only' version. 86 HP.  A few minor chassis with minor differences, called the V51, were produced. [LINDH]"]
["PV656",1936,"PV656frame",null,null,"EC",null,"manual",0,null,0,null,0,"80 HP, frame only. [LINDH]"]
["PV657",1936,"PV657frame",null,null,"EC",null,"manual",0,null,0,null,0,"80 HP, frame only for ambulances. [LINDH]"]
["PV658",1936,"PV658sedan",null,null,"EC",null,"manual",0,null,0,null,0,"80 HP, base version. [LINDH]"]
["PV659",1936,"PV658sedan",null,null,"EC",null,"manual",0,null,0,null,0,"80 HP, deluxe version. [LINDH]"]
["TR701",1936,"TR671taxi",null,null,"EC",null,"manual",0,null,0,null,0,"Taxi, with partition, 80 HP. [LINDH]"]
["TR702",1936,"TR677frame",null,null,"EC",null,"manual",0,null,0,null,0,"Taxi, frame only, 80 HP. [LINDH]"]
["TR703",1936,"TR678taxi",null,null,"EC",null,"manual",0,null,0,null,0,"Taxi, with partition, 80 HP. [LINDH]"]
["TR704",1936,"TR678taxi",null,null,"EC",null,"manual",0,null,0,null,0,"Taxi, without partition, 80 HP. [LINDH]"]
["PV36",1937,"PV36sedan",null,null,"EC",null,"manual",0,null,0,null,0,"84 HP, new 'American-like' sleek steel body on frame. [LINDH]"]
["PV51",1937,"PV51sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Base version. 86 HP, steel body on frame. [LINDH]"]
["PV51ch",1937,"PV51frame",null,null,"EC",null,"manual",0,null,0,null,0,"'Frame only' version. 86 HP.  A few minor chassis with minor differences, called the V51, were produced. [LINDH]"]
["PV52",1937,"PV51sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Deluxe version of the PV51. 86 HP, steel body on frame. [LINDH]"]
["PV658",1937,"PV658sedan",null,null,"EC",null,"manual",0,null,0,null,0,"80 HP, base version. [LINDH]"]
["TR701",1937,"TR671taxi",null,null,"EC",null,"manual",0,null,0,null,0,"Taxi, with partition, 80 HP [LINDH]."]
["TR702",1937,"TR677frame",null,null,"EC",null,"manual",0,null,0,null,0,"Taxi, frame only, 80 HP. [LINDH]"]
["TR703",1937,"TR678taxi",null,null,"EC",null,"manual",0,null,0,null,0,"Taxi, with partition, 80 HP. [LINDH]"]
["TR704",1937,"TR678taxi",null,null,"EC",null,"manual",0,null,0,null,0,"Taxi, without partition, 80 HP. [LINDH]"]
["PV36",1938,"PV36sedan",null,null,"EC",null,"manual",0,null,0,null,0,"84 HP, new 'American-like' sleek steel body on frame. [LINDH]"]
["PV51",1938,"PV51sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Base version. 86 HP, steel body on frame. [LINDH]"]
["PV51ch",1938,"PV51frame",null,null,"EC",null,"manual",0,null,0,null,0,"'Frame only' version. 86 HP. [LINDH]"]
["PV52",1938,"PV51sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Deluxe version of the PV51. 86 HP, steel body on frame. [LINDH]"]
["PV53",1938,"PV53sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Base version. 86 HP, spare tire in boot lid. [LINDH]"]
["PV54",1938,"PV54sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Base version. 86 HP, spare tire in enlarged boot. [LINDH]"]
["PV55",1938,"PV53sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Deluxe version. 86 HP, spare tire in boot lid. [LINDH]"]
["PV56",1938,"PV54sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Deluxe version. 86 HP, spare tire in enlarged boot. [LINDH]"]
["PV56ch",1938,"PV56frame",null,null,"ECG",null,"manual",0,null,0,null,0,"'Frame only' version. 50 HP Producer Gas engine. [LINDH]"]
["PV800",1938,"PV801taxi","PV802taxi",null,"EC",null,"manual",0,null,0,null,0,"Taxi, 801 = with partition, 802 = without partition, 86 HP, except ECG producer gas 50 HP engine during the war. [LINDH]"]
["PV810",1938,null,null,"PV810frame","EC",null,"manual",0,null,0,null,0,"Long wheelbase frame 'only version', 86 HP, except ECG producer gas 50 HP engine during the war. [LINDH]"]
["PV53",1939,"PV53sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Base version. 86 HP, spare tire in boot lid. [LINDH]"]
["PV54",1939,"PV54sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Base version. 86 HP, spare tire in enlarged boot. [LINDH]"]
["PV55",1939,"PV53sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Deluxe version. 86 HP, spare tire in boot lid. [LINDH]"]
["PV56",1939,"PV54sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Deluxe version. 86 HP, spare tire in enlarged boot. [LINDH]"]
["PV56ch",1939,"PV56frame",null,null,"ECG",null,"manual",0,null,0,null,0,"'Frame only' version. 50 HP Producer Gas engine. [LINDH]"]
["PV800",1939,"PV801taxi","PV802taxi","PV800frame","EC",null,"manual",0,null,0,null,0,"Taxi, 801 = with partition, 802 = without partition, 86 HP, except ECG producer gas 50 HP engine during the war. [LINDH]"]
["PV810",1939,null,null,"PV810frame","EC",null,"manual",0,null,0,null,0,"Long wheelbase frame 'only version', 86 HP, except ECG producer gas 50 HP engine during the war. [LINDH]"]
["PV53",1940,"PV53sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Base version. 86 HP, spare tire in boot lid. [LINDH]"]
["PV54",1940,"PV54sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Base version. 86 HP, spare tire in enlarged boot. [LINDH]"]
["PV55",1940,"PV53sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Deluxe version. 86 HP, spare tire in boot lid. [LINDH]"]
["PV56",1940,"PV54sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Deluxe version. 86 HP, spare tire in enlarged boot. [LINDH]"]
["PV56ch",1940,"PV56frame",null,null,"ECG",null,"manual",0,null,0,null,0,"'Frame only' version. 50 HP Producer Gas engine. [LINDH]"]
["PV800",1940,"PV801taxi","PV802taxi","PV800frame","EC",null,"manual",0,null,0,null,0,"Taxi, 801 = with partition, 802 = without partition, 86 HP, except ECG producer gas 50 HP engine during the war. [LINDH]"]
["PV810",1940,null,null,"PV810frame","EC",null,"manual",0,null,0,null,0,"Long wheelbase frame 'only version', 86 HP, except ECG producer gas 50 HP engine during the war. [LINDH]"]
["PV53",1941,"PV53sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Base version. 86 HP, spare tire in boot lid. [LINDH]"]
["PV54",1941,"PV54sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Base version. 86 HP, spare tire in enlarged boot. [LINDH]"]
["PV55",1941,"PV53sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Deluxe version. 86 HP, spare tire in boot lid. [LINDH]"]
["PV56",1941,"PV54sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Deluxe version. 86 HP, spare tire in enlarged boot. [LINDH]"]
["PV56ch",1941,"PV56frame",null,null,"ECG",null,"manual",0,null,0,null,0,"'Frame only' version. 50 HP Producer Gas engine. [LINDH]"]
["PV800",1941,"PV801taxi","PV802taxi","PV800frame","EC",null,"manual",0,null,0,null,0,"Taxi, 801 = with partition, 802 = without partition, 86 HP, except ECG producer gas 50 HP engine during the war. [LINDH]"]
["PV810",1941,null,null,"PV810frame","EC",null,"manual",0,null,0,null,0,"Long wheelbase frame 'only version', 86 HP, except ECG producer gas 50 HP engine during the war. [LINDH]"]
["PV53",1942,"PV53sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Base version. 86 HP, spare tire in boot lid. [LINDH]"]
["PV54",1942,"PV54sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Base version. 86 HP, spare tire in enlarged boot. [LINDH]"]
["PV55",1942,"PV53sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Deluxe version. 86 HP, spare tire in boot lid. [LINDH]"]
["PV56",1942,"PV54sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Deluxe version. 86 HP, spare tire in enlarged boot. [LINDH]"]
["PV56ch",1942,"PV56frame",null,null,"ECG",null,"manual",0,null,0,null,0,"'Frame only' version. 50 HP Producer Gas engine. [LINDH]"]
["PV800",1942,"PV801taxi","PV802taxi","PV800frame","EC",null,"manual",0,null,0,null,0,"Taxi, 801 = with partition, 802 = without partition, 86 HP, except ECG producer gas 50 HP engine during the war. [LINDH]"]
["PV810",1942,null,null,"PV810frame","EC",null,"manual",0,null,0,null,0,"Long wheelbase frame 'only version', 86 HP, except ECG producer gas 50 HP engine during the war. [LINDH]"]
["PV53",1943,"PV53sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Base version. 86 HP, spare tire in boot lid. [LINDH]"]
["PV54",1943,"PV54sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Base version. 86 HP, spare tire in enlarged boot. [LINDH]"]
["PV55",1943,"PV53sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Deluxe version. 86 HP, spare tire in boot lid. [LINDH]"]
["PV56",1943,"PV54sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Deluxe version. 86 HP, spare tire in enlarged boot. [LINDH]"]
["PV56ch",1943,"PV56frame",null,null,"ECG",null,"manual",0,null,0,null,0,"'Frame only' version. 50 HP Producer Gas engine. [LINDH]"]
["PV800",1943,"PV801taxi","PV802taxi","PV800frame","EC",null,"manual",0,null,0,null,0,"Taxi, 801 = with partition, 802 = without partition, 86 HP, except ECG producer gas 50 HP engine during the war. [LINDH]"]
["PV810",1943,null,null,"PV810frame","EC",null,"manual",0,null,0,null,0,"Long wheelbase frame 'only version', 86 HP, except ECG producer gas 50 HP engine during the war. [LINDH]"]
["444",1944,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"44 HP, UK?"]
["PV53",1944,"PV53sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Base version. 86 HP, spare tire in boot lid. [LINDH]"]
["PV54",1944,"PV54sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Base version. 86 HP, spare tire in enlarged boot. [LINDH]"]
["PV55",1944,"PV53sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Deluxe version. 86 HP, spare tire in boot lid. [LINDH]"]
["PV56",1944,"PV54sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Deluxe version. 86 HP, spare tire in enlarged boot. [LINDH]"]
["PV56ch",1944,"PV56frame",null,null,"ECG",null,"manual",0,null,0,null,0,"'Frame only' version. 50 HP Producer Gas engine. [LINDH]"]
["PV800",1944,"PV801taxi","PV802taxi","PV800frame","EC",null,"manual",0,null,0,null,0,"Taxi, 801 = with partition, 802 = without partition, 86 HP, except ECG producer gas 50 HP engine during the war."]
["PV810",1944,null,null,"PV810frame","EC",null,"manual",0,null,0,null,0,"Long wheelbase frame 'only version', 86 HP, except ECG producer gas 50 HP engine during the war. [LINDH]"]
["444",1945,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"44 HP, UK?"]
["PV53",1945,"PV53sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Base version. 86 HP, spare tire in boot lid. [LINDH]"]
["PV54",1945,"PV54sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Base version. 86 HP, spare tire in enlarged boot. [LINDH]"]
["PV55",1945,"PV53sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Deluxe version. 86 HP, spare tire in boot lid. [LINDH]"]
["PV56",1945,"PV54sedan",null,null,"EC",null,"manual",0,null,0,null,0,"Deluxe version. 86 HP, spare tire in enlarged boot. [LINDH]"]
["PV56ch",1945,"PV56frame",null,null,"ECG",null,"manual",0,null,0,null,0,"'Frame only' version. 50 HP Producer Gas engine. [LINDH]"]
["PV800",1945,"PV801taxi","PV802taxi","PV800frame","EC",null,"manual",0,null,0,null,0,"Taxi, 801 = with partition, 802 = without partition, 86 HP, except ECG producer gas 50 HP engine during the war. [LINDH]"]
["PV810",1945,null,null,"PV810frame","EC",null,"manual",0,null,0,null,0,"Long wheelbase frame 'only version', 86 HP, except ECG producer gas 50 HP engine during the war. [LINDH]"]
["444",1946,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"44 HP, UK?"]
["PV60",1946,"PV60sedan",null,null,"ED",null,"manual",0,null,0,null,0,"90 HP."]
["PV61",1946,"PV61frame",null,null,"ED",null,"manual",0,null,0,null,0,"90 HP."]
["PV800",1946,"PV801taxi","PV802taxi","PV800frame","EC",null,"manual",0,null,0,null,0,"Taxi, 801 = with partition, 802 = without partition, 86 HP, except ECG producer gas 50 HP engine during the war. [LINDH]"]
["PV810",1946,null,null,"PV810frame","EC",null,"manual",0,null,0,null,0,"Long wheelbase frame 'only version', 86 HP, except ECG producer gas 50 HP engine during the war. [LINDH]"]
["444",1947,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"44 HP, UK?"]
["444 Sport",1947,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"The 444 Sport identifies a 444 with more luxurious trim. [VLVWORLD]"]
["PV60",1947,"PV60sedan",null,null,"ED",null,"manual",0,null,0,null,0,"90 HP. [LINDH]"]
["PV61",1947,"PV61frame",null,null,"ED",null,"manual",0,null,0,null,0,"90 HP. [LINDH]"]
["PV800",1947,"PV801taxi","PV802taxi","PV800frame","EC",null,"manual",0,null,0,null,0,"Taxi, 801 = with partition, 802 = without partition, 86 HP, except ECG producer gas 50 HP engine during the war. [LINDH]"]
["PV810",1947,null,null,"PV810frame","EC",null,"manual",0,null,0,null,0,"Long wheelbase frame 'only version', 86 HP, except ECG producer gas 50 HP engine during the war. [LINDH]"]
["PV820",1947,null,"PV822taxi","PV825frame","ED",null,"manual",0,null,0,null,0,"Taxi, PV821 = with partition, PV822 = without partition, PV825 = 'frame only', 90 HP. [LINDH]"]
["444",1948,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"44 HP, UK?"]
["444 Sport",1948,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"The 444 Sport identifies a 444 with more luxurious trim. [VLVWORLD]"]
["PV60",1948,"PV60sedan",null,null,"ED",null,"manual",0,null,0,null,0,"90 HP. [LINDH]"]
["PV61",1948,"PV61frame",null,null,"ED",null,"manual",0,null,0,null,0,"90 HP. [LINDH]"]
["PV820",1948,"PV821taxi","PV822taxi","PV825frame","ED",null,"manual",0,null,0,null,0,"Taxi, PV821 = with partition, PV822 = without partition, PV825 = 'frame only', 90 HP. [LINDH]"]
["444",1949,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"44 HP, UK?"]
["444 Sport",1949,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"The 444 Sport identifies a 444 with more luxurious trim. [VLVWORLD]"]
["PV60",1949,"PV60sedan",null,null,"ED",null,"manual",0,null,0,null,0,"90 HP. [LINDH]"]
["PV61",1949,"PV61frame",null,null,"ED",null,"manual",0,null,0,null,0,"90 HP. [LINDH]"]
["444",1950,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"44 HP, UK?"]
["444 Sport",1950,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"The 444 Sport identifies a 444 with more luxurious trim. [VLVWORLD]"]
["PV60",1950,"PV60sedan",null,null,"ED",null,"manual",0,null,0,null,0,"90 HP. [LINDH]"]
["PV61",1950,"PV61frame",null,null,"ED",null,"manual",0,null,0,null,0,"90 HP. [LINDH]"]
["PV830",1950,"PV831taxi","PV832taxi","PV835frame","ED",null,"manual",0,null,0,null,0,"Taxi, PV831 = with partition, PV832 = without partition, PV835 = 'frame only', 90 HP. [LINDH]"]
["444",1951,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"44 HP, UK?"]
["444 Sport",1951,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"The 444 Sport identifies a 444 with more luxurious trim. [VLVWORLD]"]
["PV830",1951,"PV831taxi","PV832taxi","PV835frame","ED",null,"manual",0,null,0,null,0,"Taxi, PV831 = with partition, PV832 = without partition, PV835 = 'frame only', 90 HP. [LINDH]"]
["444",1952,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"44 HP, UK?"]
["444 Sport",1952,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"The 444 Sport identifies a 444 with more luxurious trim. [VLVWORLD]"]
["PV830",1952,"PV831taxi","PV832taxi","PV835frame","ED",null,"manual",0,null,0,null,0,"Taxi, PV831 = with partition, PV832 = without partition, PV835 = 'frame only', 90 HP. [LINDH]"]
["444",1953,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"44 HP, UK?"]
["444 Sport",1953,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"The 444 Sport identifies a 444 with more luxurious trim. [VLVWORLD]"]
["445",1953,"445wagon","445pickup","445van","B4B",null,"M3",0,"M4",0,null,0,"44 HP, UK?"]
["PV830",1953,"PV831taxi","PV832taxi","PV835frame","ED",null,"manual",0,null,0,null,0,"Taxi, PV831 = with partition, PV832 = without partition, PV835 = 'frame only', 90 HP. [LINDH]"]
["444",1954,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"44 HP, UK?"]
["444 Sport",1954,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"The 444 Sport identifies a 444 with more luxurious trim. [VLVWORLD]"]
["445",1954,"445wagon","445pickup","445van","B4B",null,"M3",0,"M4",0,null,0,"44 HP, UK?"]
["PV830",1954,"PV831taxi","PV832taxi","PV835frame","ED",null,"manual",0,null,0,null,0,"Taxi, PV831 = with partition, PV832 = without partition, PV835 = 'frame only', 90 HP. [LINDH]"]
["444",1955,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"51 HP, UK?"]
["444 Sport",1955,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"The 444 Sport identifies a 444 with more luxurious trim. [VLVWORLD]"]
["444 Sport (US)",1955,"444sedan",null,null,"B14A",null,"M3",0,"M4",0,null,0,"US version, the 444 Sport identifies a 444 with more luxurious trim. [VLVWORLD]"]
["445",1955,"445wagon","445pickup","445van","B4B",null,"M3",0,"M4",0,null,0,"44 HP, UK?"]
["PV830",1955,"PV831taxi","PV832taxi","PV835frame","ED",null,"manual",0,null,0,null,0,"Taxi, PV831 = with partition, PV832 = without partition, PV835 = 'frame only', 90 HP. [LINDH]"]
["444",1956,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"51 HP, UK?"]
["444 Sport",1956,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"The 444 Sport identifies a 444 with more luxurious trim. [VLVWORLD]"]
["444 Sport (US)",1956,"444sedan",null,null,"B14A",null,"M3",0,"M4",0,null,0,"US version, the 444 Sport identifies a 444 with more luxurious trim. [VLVWORLD]"]
["445",1956,"445wagon","445pickup","445van","B4B",null,"M3",0,"M4",0,null,0,"51 HP, UK?"]
["Amazon",1956,"120sedan",null,null,"B16A",null,"H6",0,null,0,null,0,"First name given to the 120 series, name dropped after a German motorcycle manufacturer successfully prevented Volvo from using their name. [VLVWORLD]"]
["P1900",1956,"P1900",null,null,"B14A",null,"manual",0,null,0,null,0,"The P1900 was the first Volvo sports car.  Not successful.  70 HP.  Fibreglass body.  Dual SU carbs."]
["PV830",1956,"PV831taxi","PV832taxi","PV835frame","ED",null,"manual",0,null,0,null,0,"Taxi, PV831 = with partition, PV832 = without partition, PV835 = 'frame only', 90 HP. [LINDH]"]
["444",1957,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"60 HP, UK?"]
["444 Sport",1957,"444sedan",null,null,"B16A",null,"M3",0,"M4",0,null,0,"The 444 Sport identifies a 444 with more luxurious trim. [VLVWORLD]"]
["444 Sport (US)",1957,"444sedan",null,null,"B16B",null,"M3",0,"M4",0,null,0,"US version, the 444 Sport identifies a 444 with more luxurious trim. [VLVWORLD]"]
["445",1957,"445wagon","445pickup","445van","B4B",null,"M3",0,"M4",0,null,0,"60 HP, UK?"]
["Amazon",1957,"120sedan",null,null,"B16A",null,"H6",0,null,0,null,0,"First name given to the 120 series, name dropped after a German motorcycle manufacturer successfully prevented Volvo from using their name. [VLVWORLD]"]
["P1900",1957,"P1900",null,null,"B14A",null,"manual",0,null,0,null,0,"The P1900 was the first Volvo sports car.  Not successful.  70 HP.  Fibreglass body.  Dual SU carbs."]
["PV830",1957,"PV831taxi","PV832taxi","PV835frame","ED",null,"manual",0,null,0,null,0,"Taxi, PV831 = with partition, PV832 = without partition, PV835 = 'frame only', 90 HP. [LINDH]"]
["444",1958,"444sedan",null,null,"B4B",null,"M3",0,"M4",0,null,0,"60 HP, UK?"]
["444 Sport",1958,"444sedan",null,null,"B16A",null,"M3",0,"M4",0,null,0,"The 444 Sport identifies a 444 with more luxurious trim. [VLVWORLD]"]
["444 Sport (US)",1958,"444sedan",null,null,"B16B",null,"M3",0,"M4",0,null,0,"US version, the 444 Sport identifies a 444 with more luxurious trim. [VLVWORLD]"]
["445",1958,"445wagon","445pickup","445van","B4B",null,"M3",0,"M4",0,null,0,"60 HP, UK?"]
["Amazon",1958,"120sedan",null,null,"B16A",null,"M4",0,null,0,null,0,"First name given to the 120 series, name dropped after a German motorcycle manufacturer successfully prevented Volvo from using their name. [VLVWORLD]"]
["PV830",1958,null,null,"PV835frame","ED",null,"manual",0,null,0,null,0,"Taxi, for this final year only the PV835 (frame only) was produced, 90 HP. [LINDH]"]
["121 (4dr)",1959,"120sedan",null,null,"B16A",null,"M4",0,null,0,null,0,"Not available in the USA. [VLVWORLD]"]
["122S (4dr)",1959,"120sedan",null,null,"B16B",null,"M4",0,null,0,null,0,"[VLVWORLD]"]
["445",1959,"445wagon","445pickup","445van","B4B",null,"M3",0,"M4",0,null,0,"60 HP, UK?"]
["544 Sport",1959,"544sedan",null,null,"B16A",null,"M3",0,"M4",0,null,0,"The 544 Sport identifies a 544 with more luxurious trim. [VLVWORLD]"]
["544 Sport (US)",1959,"544sedan",null,null,"B16B",null,"M3",0,"M4",0,null,0,"US version, the 544 Sport identifies a 544 with more luxurious trim. [VLVWORLD]"]
["121 (4dr)",1960,"120sedan",null,null,"B16A",null,"M4",0,null,0,null,0,"Not available in the USA. [VLVWORLD]"]
["122S (4dr)",1960,"120sedan",null,null,"B16B",null,"M4",0,null,0,null,0,"[VLVWORLD]"]
["445",1960,"445wagon","445pickup","445van","B4B",null,"M3",0,"M4",0,null,0,"60 HP, UK?"]
["544 Sport",1960,"544sedan",null,null,"B16A",null,"M3",0,"M4",0,null,0,"The 544 Sport identifies a 544 with more luxurious trim. [VLVWORLD]"]
["544 Sport (US)",1960,"544sedan",null,null,"B16B",null,"M3",0,"M4",0,null,0,"US version, the 544 Sport identifies a 544 with more luxurious trim. [VLVWORLD]"]
["121 (4dr)",1961,"120sedan",null,null,"B16A",null,"M30",0,"M31",0,"M40",0,"Not available in the USA. [VLVWORLD]"]
["122S (4dr)",1961,"120sedan",null,null,"B16B",null,null,0,"M31",0,"M40",0,"[VLVWORLD]"]
["210",1961,"210wagon",null,null,"B16B",null,"M40",0,null,0,null,0,"6 volt electrical system. [VLVWORLD]"]
["544 Sport",1961,"544sedan",null,null,"B16A",null,"M30",0,"M40",0,null,0,"The 544 Sport identifies a 544 with more luxurious trim. 6 volt electrical system.  [VLVWORLD]"]
["544 Sport (US)",1961,"544sedan",null,null,"B16B",null,"M30",0,"M40",0,null,0,"US version, the 544 Sport identifies a 544 with more luxurious trim. 6 volt electrical system. [VLVWORLD]"]
["P1800",1961,"1800coupe",null,null,"B18B",null,"M40",0,"M41",0,null,0,"Produced in England by Jensen. [VLVWORLD]"]
["121 (2dr)",1962,"130sedan",null,null,"B18A",null,"M40",0,null,0,null,0,"Not available in the USA. [VLVWORLD]"]
["121 (4dr wagon)",1962,"220wagon",null,null,"B18A",null,"M40",0,null,0,null,0,"Not available in the USA. [VLVWORLD]"]
["121 (4dr)",1962,"120sedan",null,null,"B18A",null,"M30",0,"M40",0,null,0,"Not available in the USA. [VLVWORLD]"]
["122S (4dr)",1962,"120sedan",null,null,"B18D",null,"M40",0,"M41",0,null,0,"[VLVWORLD], [CLARKE70]"]
["210",1962,"210wagon",null,null,"B18A",null,"M40",0,null,0,null,0,"Switch from 6 to 12 volt electrical system. [VLVWORLD]"]
["544 Sport",1962,"544sedan",null,null,"B18A",null,"M30",0,"M40",0,null,0,"The 544 Sport identifies a 544 with more luxurious trim. Switch from 6 to 12 volt electrical system. [VLVWORLD]"]
["544 Sport (US)",1962,"544sedan",null,null,"B18D",null,"M30",0,"M40",0,null,0,"US version, the 544 Sport identifies a 544 with more luxurious trim. Switch from 6 to 12 volt electrical system. [VLVWORLD]"]
["P1800",1962,"1800coupe",null,null,"B18B",null,"M40",0,"M41",0,null,0,"Produced in England by Jensen. [VLVWORLD]"]
["121 (2dr)",1963,"130sedan",null,null,"B18A",null,"M30",0,null,0,null,0,"Not available in the USA. [VLVWORLD]"]
["121 (4dr wagon)",1963,"220wagon",null,null,"B18A",null,"M40",0,null,0,null,0,"Not available in the USA. [VLVWORLD]"]
["121 (4dr)",1963,"120sedan",null,null,"B18A",null,"M40",0,null,0,null,0,"Not available in the USA. [VLVWORLD]"]
["122S (2dr)",1963,"130sedan",null,null,"B18D",null,"M40",0,null,0,null,0,"[VLVWORLD]"]
["122S (4dr)",1963,"120sedan",null,null,"B18D",null,"M41",0,null,0,null,0,"[VLVWORLD]"]
["1800S",1963,"1800coupe",null,null,"B18B",null,"M40",0,"M41",0,null,0,"[VLVWORLD]"]
["210",1963,"210wagon",null,null,"B18A",null,"M40",0,null,0,null,0,"[VLVWORLD]"]
["544 Sport",1963,"544sedan",null,null,"B18A",null,"M30",0,"M40",0,null,0,"The 544 Sport identifies a 544 with more luxurious trim. [VLVWORLD]"]
["544 Sport (US)",1963,"544sedan",null,null,"B18D",null,"M30",0,"M40",0,null,0,"US version, the 544 Sport identifies a 544 with more luxurious trim. [VLVWORLD]"]
["P1800",1963,"1800coupe",null,null,"B18B",null,"M40",0,"M41",0,null,0,"Produced in England by Jensen. [VLVWORLD]"]
["121 (2dr)",1964,"130sedan",null,null,"B18A",null,"M40",0,"M41",0,null,0,"Not available in the USA. [VLVWORLD]"]
["121 (4dr wagon)",1964,"220wagon",null,null,"B18A",null,"M40",0,null,0,null,0,"Not available in the USA. [VLVWORLD]"]
["121 (4dr)",1964,"120sedan",null,null,"B18A",null,"M40",0,"M41",0,"BW35",0,"Not available in the USA. [VLVWORLD]"]
["122S (2dr)",1964,"130sedan",null,null,"B18D",null,"M40",0,"M41",0,null,0,"[VLVWORLD]"]
["122S (4dr)",1964,"120sedan",null,null,"B18D",null,"M40",0,"M41",0,"BW35",0]
["1800S",1964,"1800coupe",null,null,"B18B",null,"M41",0,null,0,null,0,"[VLVWORLD]"]
["210",1964,"210wagon",null,null,"B18A",null,"M40",0,null,0,null,0,"[VLVWORLD]"]
["544 Sport",1964,"544sedan",null,null,"B18A",null,"M30",0,"M40",0,null,0,"The 544 Sport identifies a 544 with more luxurious trim. [VLVWORLD]"]
["544 Sport (US)",1964,"544sedan",null,null,"B18D",null,"M30",0,"M40",0,null,0,"US version, the 544 Sport identifies a 544 with more luxurious trim. [VLVWORLD]"]
["121 (2dr)",1965,"130sedan",null,null,"B18A",null,"M40",0,"M41",0,null,0,"Not available in the USA. [VLVWORLD]"]
["121 (4dr wagon)",1965,"220wagon",null,null,"B18A",null,"M40",0,null,0,null,0,"Not available in the USA. [VLVWORLD]"]
["121 (4dr)",1965,"120sedan",null,null,"B18A",null,"M40",0,"M41",0,"BW35",0,"Not available in the USA. [VLVWORLD]"]
["122S (2dr)",1965,"130sedan",null,null,"B18D",null,"M40",0,"M41",0,null,0,"[VLVWORLD]"]
["122S (4dr wagon)",1965,"220wagon",null,null,"B18D",null,"M40",0,"BW35",0,null,0,"95 HP, automatic ransmission available in the US. [VLVWORLD], [USWEB1]"]
["122S (4dr)",1965,"120sedan",null,null,"B18D",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["1800S",1965,"1800coupe",null,null,"B18B",null,"M41",0,null,0,null,0,"[VLVWORLD]"]
["210",1965,"210wagon",null,null,"B18A",null,"M40",0,null,0,null,0,"[VLVWORLD]"]
["544 Sport",1965,"544sedan",null,null,"B18A",null,"M30",0,"M40",0,null,0,"The 544 Sport identifies a 544 with more luxurious trim. [VLVWORLD]"]
["544 Sport (US)",1965,"544sedan",null,null,"B18D",null,"M30",0,"M40",0,null,0,"US version, the 544 Sport identifies a 544 with more luxurious trim. [VLVWORLD]"]
["121 (2dr)",1966,"130sedan",null,null,"B18A",null,"M40",0,"M41",0,"BW35",0,"Not available in the USA. [VLVWORLD]"]
["121 (4dr wagon)",1966,"220wagon",null,null,"B18A",null,"M40",0,null,0,null,0,"Not available in the USA. [VLVWORLD]"]
["121 (4dr)",1966,"120sedan",null,null,"B18A",null,"M40",0,"M41",0,"BW35",0,"Not available in the USA. [VLVWORLD]"]
["122S (2dr)",1966,"130sedan",null,null,"B18D",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["122S (4dr wagon)",1966,"220wagon",null,null,"B18D",null,"M40",0,null,0,null,0,"[VLVWORLD]"]
["122S (4dr)",1966,"120sedan",null,null,"B18D",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["1800S",1966,"1800coupe",null,null,"B18B",null,"M41",0,null,0,null,0,"[VLVWORLD]"]
["210",1966,"210wagon",null,null,"B18A",null,"M40",0,null,0,null,0,"[VLVWORLD]"]
["544 Sport",1966,"544sedan",null,null,"B18A",null,"M30",0,"M40",0,null,0,"The 544 Sport identifies a 544 with more luxurious trim. [VLVWORLD]"]
["544 Sport (US)",1966,"544sedan",null,null,"B18D",null,"M30",0,"M40",0,null,0,"US version, the 544 Sport identifies a 544 with more luxurious trim. [VLVWORLD]"]
["121 (2dr)",1967,"130sedan",null,null,"B18A",null,"M40",0,null,0,"BW35",0,"Not available in the USA. [VLVWORLD]"]
["121 (4dr wagon)",1967,"220wagon",null,null,"B18A",null,"M40",0,null,0,null,0,"Not available in the USA. [VLVWORLD]"]
["121 (4dr)",1967,"120sedan",null,null,"B18A",null,"M40",0,"M41",0,"BW35",0,"Not available in the USA. [VLVWORLD]"]
["122S (2dr)",1967,"130sedan",null,null,"B18D",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["122S (4dr wagon)",1967,"220wagon",null,null,"B18D",null,"M40",0,null,0,null,0,"[VLVWORLD]"]
["122S (4dr)",1967,"120sedan",null,null,"B18D",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["123GT",1967,"130sedan",null,null,"B18B",null,"M41",0,null,0,null,0,"Sports trim. [VLVWORLD]"]
["142",1967,"142sedan",null,null,"B18A",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["142S",1967,"142sedan",null,null,"B18B",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["144",1967,"144sedan",null,null,"B18A",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["144S",1967,"144sedan",null,null,"B18B",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["1800S",1967,"1800coupe",null,null,"B18B",null,"M41",0,null,0,null,0,"[VLVWORLD]"]
["210",1967,"210wagon",null,null,"B18A",null,null,0,"M40",0,null,0,"[VLVWORLD]"]
["121 (2dr)",1968,"130sedan",null,null,"B18A",null,"M30",0,"M40",0,"BW35",0,"Not available in the USA. [VLVWORLD]"]
["121 (4dr wagon)",1968,"220wagon",null,null,"B18A",null,"M40",0,null,0,"BW35",0,"Not available in the USA. [VLVWORLD]"]
["122S (2dr)",1968,"130sedan",null,null,"B18B",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["122S (4dr wagon)",1968,"220wagon",null,null,"B18B",null,"M40",0,null,0,"BW35",0,"[VLVWORLD]"]
["123GT",1968,"130sedan",null,null,"B18B",null,"M41",0,null,0,null,0,"Sports trim. [VLVWORLD]"]
["142",1968,"142sedan",null,null,"B18A",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["142S",1968,"142sedan",null,null,"B18B",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["144",1968,"144sedan",null,null,"B18A",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["144S",1968,"144sedan",null,null,"B18B",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["145S",1968,"145wagon",null,null,"B18B",null,"M40",0,null,0,"BW35",0,"[VLVWORLD]"]
["1800S",1968,"1800coupe",null,null,"B18B",null,"M41",0,null,0,null,0,"[VLVWORLD]"]
["210",1968,"210wagon",null,null,"B18A",null,"M40",0,null,0,null,0,"[VLVWORLD]"]
["121 (2dr)",1969,"130sedan",null,null,"B20A",null,"M40",0,null,0,null,0,"Not available in the USA. [VLVWORLD]"]
["121 (4dr wagon)",1969,"220wagon",null,null,"B20A",null,"M40",0,null,0,null,0,"Not available in the USA. [VLVWORLD]"]
["122S (2dr)",1969,"130sedan",null,null,"B20B",null,"M40",0,null,0,null,0,"[VLVWORLD]"]
["142",1969,"142sedan",null,null,"B20A",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["142S",1969,"142sedan",null,null,"B20B",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["144",1969,"144sedan",null,null,"B20A",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["144S",1969,"144sedan",null,null,"B20B",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["145",1969,"145wagon",null,null,"B20A",null,"M40",0,null,0,"BW35",0,"[VLVWORLD]"]
["145S",1969,"145wagon",null,null,"B20B",null,"M40",0,null,0,"BW35",0,"[VLVWORLD]"]
["164",1969,"164sedan",null,null,"B30A",null,"M400",0,null,0,"BW35",0,"[VLVWORLD]"]
["1800S",1969,"1800coupe",null,null,"B20B",null,"M41",0,null,0,null,0,"[VLVWORLD]"]
["210",1969,"210wagon",null,null,"B18A",null,"M40",0,null,0,null,0,"[VLVWORLD]"]
["121 (2dr)",1970,"130sedan",null,null,"B20A",null,"M40",0,null,0,null,0,"Not available in the USA. [VLVWORLD]"]
["122S (2dr)",1970,"130sedan",null,null,"B20B",null,"M40",0,null,0,null,0,"[VLVWORLD]"]
["142",1970,"142sedan",null,null,"B20A",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["142S",1970,"142sedan",null,null,"B20B",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["144",1970,"144sedan",null,null,"B20A",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["144S",1970,"144sedan",null,null,"B20B",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["145",1970,"145wagon",null,null,"B20A",null,"M40",0,null,0,"BW35",0,"[VLVWORLD]"]
["145S",1970,"145wagon",null,null,"B20B",null,"M40",0,null,0,"BW35",0,"[VLVWORLD]"]
["164",1970,"164sedan",null,null,"B30A",null,"M400",0,null,0,"BW35",0,"[VLVWORLD]"]
["1800E",1970,"1800coupe",null,null,"B20E",null,"M41",0,"M410",0,null,0,"[VLVWORLD]"]
["142E",1971,"142sedan",null,null,"B20E",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["142S",1971,"142sedan",null,null,"B20B",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["144",1971,"144sedan",null,null,"B20A",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["144S",1971,"144sedan",null,null,"B20B",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["145",1971,"145wagon",null,null,"B20A",null,"M40",0,null,0,"BW35",0,"[VLVWORLD]"]
["145S",1971,"145wagon",null,null,"B20B",null,"M40",0,null,0,"BW35",0,"[VLVWORLD]"]
["164",1971,"164sedan",null,null,"B30A",null,"M400",0,null,0,"BW35",0,"[VLVWORLD]"]
["1800E",1971,"1800coupe",null,null,"B20E",null,"M41",0,"BW35",0,null,0,"[VLVWORLD]"]
["142E (non USA)",1972,"142sedan",null,null,"B20E",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["142E (USA)",1972,"142sedan",null,null,"B20F",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["142S",1972,"142sedan",null,null,"B20B",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["144E",1972,"144sedan",null,null,"B20F",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["144S",1972,"144sedan",null,null,"B20B",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["145E",1972,"145wagon",null,null,"B20F",null,"M40",0,null,0,"BW35",0,"[VLVWORLD]"]
["145S",1972,"145wagon",null,null,"B20A",null,"M40",0,null,0,"BW35",0,"[VLVWORLD]"]
["164",1972,"164sedan",null,null,"B30A",null,"M410",0,null,0,"BW35",0,"[VLVWORLD]"]
["164E",1972,"164sedan",null,null,"B30E",null,"M410",0,null,0,"BW35",0,"[VLVWORLD]"]
["1800E",1972,"1800coupe",null,null,"B20E",null,"M41",0,"BW35",0,null,0,"[VLVWORLD]"]
["1800E",1972,"1800coupe",null,null,"B20F",null,"M41",0,"BW35",0,null,0,"125 HP, Tires: 185 HR 15. [VLVWORLD]"]
["1800ES",1972,"1800wagon",null,null,"B20E",null,"M41",0,"BW35",0,null,0,"[VLVWORLD]"]
["1800ES",1972,"1800wagon",null,null,"B20F",null,"M41",0,"BW35",0,null,0,"[VLVWORLD]"]
["142E (non USA)",1973,"142sedan",null,null,"B20E",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["142E (USA)",1973,"142sedan",null,null,"B20F",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["142S (non USA)",1973,"142sedan",null,null,"B20B",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["144E",1973,"144sedan",null,null,"B20F",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["144S (non USA)",1973,"144sedan",null,null,"B20B",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["145E",1973,"145wagon",null,null,"B20F",null,"M40",0,null,0,"BW35",0,"[VLVWORLD]"]
["145S (non USA)",1973,"145wagon",null,null,"B20A",null,"M40",0,null,0,"BW35",0,"[VLVWORLD]"]
["164E",1973,"164sedan",null,null,"B30E",null,"M410",0,null,0,"BW35",0,"[VLVWORLD]"]
["164E (US?)",1973,"164sedan",null,null,"B30F",null,"M410",0,null,0,"BW35",0,"[VLVWORLD]"]
["1800ES",1973,"1800wagon",null,null,"B20E",null,"M41",0,"BW35",0,null,0,"[VLVWORLD]"]
["1800ES",1973,"1800wagon",null,null,"B20F",null,"M41",0,"BW35",0,null,0,"[VLVWORLD]"]
["142E (non USA)",1974,"142sedan",null,null,"B20E",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["142E (USA)",1974,"142sedan",null,null,"B20F",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["142S (non USA)",1974,"142sedan",null,null,"B20B",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["144E",1974,"144sedan",null,null,"B20F",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["144S (non USA)",1974,"144sedan",null,null,"B20B",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["145E",1974,"145wagon",null,null,"B20F",null,"M40",0,null,0,"BW35",0,"[VLVWORLD]"]
["145S (non USA)",1974,"145wagon",null,null,"B20A",null,"M40",0,null,0,"BW35",0,"[VLVWORLD]"]
["164E",1974,"164sedan",null,null,"B30E",null,"M410",0,null,0,"BW35",0,"[VLVWORLD]"]
["164E (US?)",1974,"164sedan",null,null,"B30F",null,"M410",0,null,0,"BW35",0,"[VLVWORLD]"]
["164E",1975,"164sedan",null,null,"B30E",null,"M410",0,null,0,"BW35",0,"[VLVWORLD]"]
["164E (US?)",1975,"164sedan",null,null,"B30F",null,"M410",0,null,0,"BW35",0,"[VLVWORLD]"]
["240 DL",1975,"242sedan","244sedan","245wagon","B20F",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["240 GL",1975,"242sedan","244sedan",null,"B20F",null,"M40",0,"M41",0,"BW35",0,"[VLVWORLD]"]
["260 GL",1975,"264sedan",null,null,"B27F V6",null,"M46",0,null,0,"BW55",0,"[VLVWORLD]"]
["66",1975,"66sedan","66combi",{"$nulls":4},0,null,0,null,0,"Small car of DAF origins, poor quality."]
["240 DL",1976,"242sedan","244sedan","245wagon","B21F",null,"M45",0,"M46",0,"BW35",0,"[VLVWORLD]"]
["240 GL",1976,"242sedan","244sedan",null,"B21F",null,"M45",0,"M46",0,"BW35",0,"[VLVWORLD]"]
["260",1976,null,null,"265wagon","B27F V6",null,"M46",0,null,0,"BW55",0,"[VLVWORLD]"]
["260 GL",1976,"262sedan","264sedan",null,"B27F V6",null,"M46",0,null,0,"BW55",0,"[VLVWORLD]"]
["340",1976,"343hatch",null,null,"B19",null,null,0,null,0,null,0,"Small car.  Not sold in North America."]
["66",1976,"66sedan","66combi",{"$nulls":4},0,null,0,null,0,"Small car of DAF origins, poor quality.  Not sold in North America."]
["240 DL (Canada)",1977,"242sedan","244sedan","245wagon","B21A",null,"M45",0,"M46",0,"BW35",0,"[VLVWORLD]"]
["240 DL (USA)",1977,"242sedan","244sedan","245wagon","B21F",null,"M45",0,"M46",0,"BW35",0,"[VLVWORLD]"]
["240 GL",1977,"242sedan","244sedan",null,"B21F",null,"M45",0,"M46",0,"BW35",0,"[VLVWORLD]"]
["260",1977,null,null,"265wagon","B27F V6",null,"M46",0,null,0,"BW55",0,"[VLVWORLD]"]
["260 GL",1977,"262sedan","264sedan",null,"B27F V6",null,"M46",0,null,0,"BW55",0,"[VLVWORLD]"]
["340",1977,"343hatch",null,null,"B19",null,null,0,null,0,null,0,"Small car.  Not sold in North America."]
["66",1977,"66sedan","66combi",{"$nulls":4},0,null,0,null,0,"Small car of DAF origins, poor quality.  Not sold in North America."]
["240 DL (Canada)",1978,"242sedan","244sedan","245wagon","B21A",null,"M45",0,"M46",0,"BW35",0,"[VLVWORLD]"]
["240 DL (US)",1978,"242sedan","244sedan","245wagon","B21F",null,"M45",0,"M46",0,"BW35",0,"[VLVWORLD]"]
["240 GL",1978,null,"244sedan",null,"B21F",null,"M45",0,"M46",0,"BW35",0,"[VLVWORLD]"]
["240 GT (Canada)",1978,"242sedan",null,null,"B21F",null,"M45",0,"M46",0,"BW35",0,"[VLVWORLD]"]
["240 GT (US)",1978,"242sedan",null,null,"B21F",null,"M45",0,"M46",0,"BW35",0,"[VLVWORLD]"]
["260 GL",1978,"264sedan","265wagon",null,"B27F V6",null,"M46",0,null,0,"BW55",0,"[VLVWORLD]"]
["262 C",1978,null,null,"262coupe","B27F V6",null,"M46",0,null,0,"BW55",0,"[VLVWORLD]"]
["340",1978,"343hatch",null,null,"B19",null,null,0,null,0,null,0,"Small car.  Not sold in North America."]
["66",1978,"66sedan","66combi",{"$nulls":4},0,null,0,null,0,"Small car of DAF origins, poor quality.  Not sold in North America."]
["240 DL (Canada)",1979,"242sedan","244sedan","245wagon","B21A",null,"M45",0,"M46",0,"BW35",0,"AW70 transmission also available? [VLVWORLD]"]
["240 DL (US)",1979,"242sedan","244sedan","245wagon","B21F",null,"M45",0,"M46",0,"BW35",0,"AW70 transmission also available? [VLVWORLD]"]
["240 GL",1979,null,"244sedan",null,"B21F",null,"M45",0,"M46",0,"BW35",0,"AW70 transmission also available? [VLVWORLD]"]
["240 GT (Canada)",1979,"242sedan",null,null,"B21F",null,"M45",0,"M46",0,"BW35",0,"AW70 transmission also available? [VLVWORLD]"]
["240 GT (US)",1979,"242sedan",null,null,"B21F",null,"M45",0,"M46",0,"BW35",0,"AW70 transmission also available? [VLVWORLD]"]
["260 GL",1979,"264sedan","265wagon",null,"B27F V6",null,"M46",0,null,0,"BW55",0,"[VLVWORLD]"]
["262 C",1979,null,null,"262coupe","B27F V6",null,"M46",0,null,0,"BW55",0,"[VLVWORLD]"]
["340",1979,"343hatch","345wagon",null,"B19",null,null,0,null,0,null,0,"Small car.  Not sold in North America."]
["66",1979,"66sedan",{"$nulls":5},0,null,0,null,0,"Small car of DAF origins, poor quality.  Not sold in North America."]
["240 DL (Canada)",1980,"242sedan","244sedan","245wagon","B21A",null,"M45",0,"M46",0,"BW35",0,"AW70 transmission also available? [VLVWORLD]"]
["240 DL (US)",1980,"242sedan","244sedan","245wagon","B21F",null,"M45",0,"M46",0,"BW35",0,"AW70 transmission also available? [VLVWORLD]"]
["240 GL",1980,null,"244sedan","245wagon","B21F",null,"M45",0,"M46",0,"BW35",0,"AW70 transmission also available? [VLVWORLD]"]
["240 GT (Canada)",1980,"242sedan",null,null,"B21F",null,"M45",0,"M46",0,"BW35",0,"AW70 transmission also available? [VLVWORLD]"]
["240 GT (US)",1980,"242sedan",null,null,"B21F",null,"M45",0,"M46",0,"BW35",0,"AW70 transmission also available? [VLVWORLD]"]
["260 GLE",1980,"264sedan","265wagon",null,"B28F V6",null,"M46",0,null,0,"BW55",0,"[VLVWORLD]"]
["262 COUPE",1980,null,null,"262coupe","B28F V6",null,"M46",0,null,0,"BW55",0,"[VLVWORLD]"]
["340",1980,"343hatch","345wagon",null,"B19",null,null,0,null,0,null,0,"Small car.  Not sold in North America."]
["66",1980,"66sedan",{"$nulls":5},0,null,0,null,0,"Small car of DAF origins, poor quality.  Not sold in North America."]
["240 DIESEL",1981,"244sedan","245wagon",null,"D24T","Turbo","M46",0,null,0,"BW55",0,"Diesel, turbo? [VLVWORLD]"]
["240 DL (Canada)",1981,"242sedan","244sedan","245wagon","B21A",null,"M46",0,"BW55",0,"AW70",0,"[VLVWORLD]"]
["240 DL (USA)",1981,"242sedan","244sedan","245wagon","B21F",null,"M46",0,"BW55",0,"AW70",0,"[VLVWORLD]"]
["240 GL (Canada)",1981,"242sedan","244sedan","245wagon","B23E",null,"M46",0,"BW55",0,"AW70",0,"[VLVWORLD]"]
["240 GL (USA)",1981,"242sedan","244sedan","245wagon","B21F",null,"M46",0,"BW55",0,"AW70",0,"[VLVWORLD]"]
["240 GLT (Canada)",1981,"242sedan","244sedan",null,"B23E",null,"M46",0,"BW55",0,"AW70",0,"[VLVWORLD]"]
["240 GLT (USA)",1981,"242sedan","244sedan",null,"B21F",null,"M46",0,"BW55",0,"AW70",0,"[VLVWORLD]"]
["240 GLT Turbo (USA)",1981,"242sedan","244sedan",null,"B21FT","Garrett T3 turbo",null,0,null,0,"AW71",0,"127 HP, 150 ft-lb Torque. [VLVWORLD]"]
["260 DIESEL",1981,null,"265wagon",null,"D24T","Turbo",null,0,null,0,"BW55",0,"Diesel, turbo? [VLVWORLD]"]
["260 GLE",1981,"264sedan","265wagon",null,"B28F V6",null,null,0,null,0,"BW55",0,"[VLVWORLD]"]
["262 COUPE",1981,null,null,"262coupe","B28F V6",null,null,0,null,0,"BW55",0,"[VLVWORLD]"]
["340",1981,"343hatch","345wagon",null,"B19",null,null,0,null,0,null,0,"Small car.  Not sold in North America."]
["240 DIESEL",1982,"244sedan","245wagon",null,"D24T","Turbo","M46",0,null,0,"BW55",0,"Diesel, turbo? [VLVWORLD]"]
["240 DL (Canada)",1982,"242sedan","244sedan","245wagon","B21A",null,"M46",0,"BW55",0,"AW70",0,"[VLVWORLD]"]
["240 DL (USA)",1982,"242sedan","244sedan","245wagon","B21F",null,"M46",0,"BW55",0,"AW70",0,"[VLVWORLD]"]
["240 GL (Canada)",1982,"242sedan","244sedan","245wagon","B23E",null,"M46",0,"BW55",0,"AW70",0,"[VLVWORLD]"]
["240 GL (USA)",1982,"242sedan","244sedan","245wagon","B21F",null,"M46",0,"BW55",0,"AW70",0,"[VLVWORLD]"]
["240 GLT (Canada)",1982,"242sedan","244sedan","245wagon","B23E",null,"M46",0,"BW55",0,"AW70",0,"[VLVWORLD]"]
["240 GLT (USA)",1982,"242sedan","244sedan","245wagon","B21F",null,"M46",0,"BW55",0,"AW70",0,"[VLVWORLD]"]
["240 GLT Turbo (USA)",1982,"242sedan","244sedan","245wagon","B21FT","Garrett T3 turbo",null,0,null,0,"AW71",0,"127 HP, 150 ft-lb Torque. [VLVWORLD]"]
["260 DIESEL",1982,null,"265wagon",null,"D24T","Turbo",null,0,null,0,"BW55",0,"Diesel, turbo? [VLVWORLD]"]
["260 GLE",1982,"264sedan","265wagon",null,"B28F V6",null,null,0,null,0,"BW55",0,"[VLVWORLD]"]
["340",1982,"343hatch","345wagon",null,"B19",null,null,0,null,0,null,0,"Small car.  Not sold in North America."]
["760 GLE",1982,"760sedan",null,null,"B28F V6",null,"AW71",0,null,0,null,0,"First of the 700 series, transmission uncertain. [VLVWORLD]"]
["240 DIESEL",1983,"244sedan","245wagon",null,"D24T","Turbo","M46",0,null,0,"BW55",0,"Diesel, turbo? Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["240 DL (Canada)",1983,"242sedan","244sedan","245wagon","B21A",null,"M46",0,"BW55",0,"AW70",0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["240 DL (USA)",1983,"242sedan",null,null,"B23F",null,"M46",0,"BW55",0,"AW70",0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["240 DL/GL (USA)",1983,null,"244sedan","245wagon","B23F",null,"M46",0,"BW55",0,"AW70",0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["240 GL (Canada)",1983,null,"244sedan","245wagon","B23E",null,"M46",0,"BW55",0,"AW70",0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["240 GLT (Canada)",1983,"242sedan","244sedan","245wagon","B23E",null,"M46",0,"BW55",0,"AW70",0,"[VLVWORLD]"]
["240 GLT Turbo (USA)",1983,"242sedan","244sedan","245wagon","B21FT","Garrett T3 turbo","M46",0,null,0,"AW71",0,"127 HP, 150 ft-lb Torque.  Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["260 GLE",1983,null,"265wagon",null,"B28F V6",null,null,0,null,0,"BW55",0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["340",1983,"343hatch","345wagon",null,"B19",null,null,0,null,0,null,0,"Small car.  Not sold in North America."]
["360",1983,"360hatch","360sedan","360wagon","B19",null,null,0,null,0,null,0,"Small car.  Not sold in North America."]
["760 GLE",1983,"760sedan",null,null,"B28F V6",null,null,0,"AW71",0,"ZF-4HP22L",0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]. Possibly available with the ZF22 [BRYANT]."]
["760 GLE TD",1983,"760sedan",null,null,"D24T","Turbo","M46",0,null,0,null,0,"Turbo Diesel.  Wiring harness prone to deterioration, more so with the turbo because of the added heat [HARNESS]. [VLVWORLD]"]
["240 DIESEL",1984,"244sedan","245wagon",null,"D24T","Turbo","M46",0,null,0,"BW55",0,"Diesel, turbo? Wiring harness prone to deterioration, more so with the turbo because of the added heat [HARNESS]. [VLVWORLD]"]
["240 DL (Canada)",1984,"242sedan","244sedan",null,"B21A",null,"M46",0,"BW55",0,"AW70",0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["240 DL (USA)",1984,"242sedan","244sedan",null,"B23F",null,"M46",0,"BW55",0,"AW70",0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["240 GL",1984,"242sedan","244sedan","245wagon","B23F",null,"M46",0,"AW70",0,null,0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["240 GLT Turbo (USA)",1984,"242sedan","244sedan","245wagon","B21FT","Garrett T3 turbo","M46",0,null,0,"AW71",0,"127 HP, 150 ft-lb Torque.  Wiring harness prone to deterioration, more so with the turbo because of the added heat [HARNESS]. [VLVWORLD]"]
["260 GLE",1984,null,"265wagon",null,"B28F V6",null,null,0,null,0,"BW55",0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["340",1984,"343hatch","345wagon",null,"B19",null,null,0,null,0,null,0,"Small car.  Not sold in North America."]
["360",1984,"360hatch","360sedan","360wagon","B19",null,null,0,null,0,null,0,"Small car.  Not sold in North America."]
["740",1984,"740sedan",null,null,"B23F",null,null,0,null,0,null,0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["760 GLE",1984,"760sedan",null,null,"B28F V6",null,null,0,"AW71",0,null,0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["760 GLE TD",1984,"760sedan",null,null,"D24T","Turbo",null,0,"ZF-4HP22L",0,null,0,"Turbo Diesel.  Wiring harness prone to deterioration, more so with the turbo because of the added heat [HARNESS]. [VLVWORLD]"]
["760 Turbo",1984,"760sedan",null,null,"B23FT","Garrett T3 tic","M46",0,"AW71",0,null,0,"Turbo.  Wiring harness prone to deterioration, more so with the turbo because of the added heat [HARNESS]. [VLVWORLD]"]
["240 DIESEL",1985,"244sedan","245wagon",null,"D24T","Turbo",null,0,null,0,"BW55",0,"Diesel, turbo? Wiring harness prone to deterioration, more so with the turbo because of the added heat [HARNESS]. [VLVWORLD]"]
["240 DL/GL",1985,"244sedan","245wagon",null,"B230F",null,"M46",0,"AW70",0,null,0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["240 GLT Turbo (USA)",1985,null,"244sedan","245wagon","B21FTi","Garrett T3 tic","M46",0,null,0,"AW71",0,"160 HP, 180 ft-lb Torque.  Intercooled turbo. Wiring harness prone to deterioration, more so with the turbo because of the added heat [HARNESS]. [VLVWORLD]"]
["260 GLE",1985,null,"265wagon",null,"B28F V6",null,null,0,null,0,"BW55",0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["340",1985,"343hatch","345wagon",null,"B19",null,null,0,null,0,null,0,"Small car.  Not sold in North America."]
["360",1985,"360hatch","360sedan","360wagon","B19",null,null,0,null,0,null,0,"Small car.  Not sold in North America."]
["740",1985,"740sedan","740wagon",null,"B230F",null,"M46",0,"ZF-4HP22L",0,null,0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["740 Turbo",1985,"740sedan","740wagon",null,"B230FT","Garrett T3 tic","M46",0,"AW70",0,null,0,"Turbo.  Wiring harness prone to deterioration, more so with the turbo because of the added heat [HARNESS]. [VLVWORLD]"]
["760 GL",1985,"760sedan","760wagon",null,"B230F",null,"M46",0,"AW71",0,null,0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["760 GLE",1985,"760sedan","760wagon",null,"B28F V6",null,"M46",0,"AW71",0,null,0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["760 TD",1985,"760sedan","760wagon",null,"D24T","Turbo","ZF-4HP22L",0,null,0,null,0,"Turbo Diesel.  Wiring harness prone to deterioration, more so with the turbo because of the added heat [HARNESS]. [VLVWORLD]"]
["760 Turbo",1985,"760sedan","760wagon",null,"B230FT","Garrett T3 tic","M46",0,"AW71",0,null,0,"Turbo.  Wiring harness prone to deterioration, more so with the turbo because of the added heat [HARNESS]. [VLVWORLD]"]
["240 DL/GL",1986,"244sedan","245wagon",null,"B230F",null,"M46",0,"AW70",0,null,0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["340",1986,"343hatch","345wagon",null,"B19",null,null,0,null,0,null,0,"Small car.  Not sold in North America."]
["360",1986,"360hatch","360sedan","360wagon","B19",null,null,0,null,0,null,0,"Small car.  Not sold in North America."]
["480",1986,"480coupe",null,null,"B18E",null,"manual",0,null,0,null,0,"First FWD Volvo.  5 spd manual only.  Small car.  Not sold in North America."]
["740",1986,"740sedan","740wagon",null,"B230F",null,"M46",0,"ZF-4HP22L",0,null,0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["740 GLE TD",1986,"740sedan","740wagon",null,"D24T","Turbo","ZF-4HP22L",0,null,0,null,0,"Turbo Diesel.  Wiring harness prone to deterioration, more so with the turbo because of the added heat [HARNESS]. [VLVWORLD]"]
["740 Turbo",1986,"740sedan","740wagon",null,"B230FT","Garrett T3 tic","M46",0,"AW71",0,null,0,"Turbo.  Wiring harness prone to deterioration, more so with the turbo because of the added heat [HARNESS]. [VLVWORLD]"]
["760 GL",1986,"760sedan","760wagon",null,"B230F",null,"M46",0,"AW71",0,null,0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["760 GLE",1986,"760sedan","760wagon",null,"B28F V6",null,null,0,"AW71",0,null,0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["760 Turbo",1986,"760sedan","760wagon",null,"B230FT","Garrett T3 tic","M46",0,"AW71",0,null,0,"Turbo.  Wiring harness prone to deterioration, more so with the turbo because of the added heat [HARNESS]. [VLVWORLD]"]
["780 Turbo Coupe",1986,780,null,null,"B230FT","Garrett T3 tic+","AW71",0,null,0,null,0,"Turbo.  Wiring harness prone to deterioration, more so with the turbo because of the added heat [HARNESS]. [VLVWORLD]"]
["780 V-6 Coupe",1986,780,null,null,"B280F V6",null,"AW71",0,null,0,null,0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["240 DL/GL",1987,"244sedan","245wagon",null,"B230F",null,"M47",0,"AW70",0,null,0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["340",1987,"343hatch","345wagon",null,"B19",null,null,0,null,0,null,0,"Small car.  Not sold in North America."]
["360",1987,"360hatch","360sedan","360wagon","B19",null,null,0,null,0,null,0,"Small car.  Not sold in North America."]
["480",1987,"480coupe",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["740",1987,"740sedan","740wagon",null,"B230F",null,"M47",0,"ZF-4HP22L",0,null,0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["740 Turbo",1987,"740sedan","740wagon",null,"B230FT","Garrett T3 tic","M47",0,"AW71",0,null,0,"Turbo.  Wiring harness prone to deterioration, more so with the turbo because of the added heat [HARNESS]. [VLVWORLD]"]
["760 GLE",1987,"760sedan",null,null,"B280F V6",null,null,0,"AW71",0,null,0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["760 Turbo",1987,"760sedan","760wagon",null,"B230FT","Garrett T3 tic","M47",0,"AW71",0,null,0,"Turbo.  Wiring harness prone to deterioration, more so with the turbo because of the added heat [HARNESS]. [VLVWORLD]"]
["780 Turbo Coupe",1987,780,null,null,"B230FT","Garrett T3 tic+","AW71",0,null,0,null,0,"Turbo.  Wiring harness prone to deterioration, more so with the turbo because of the added heat [HARNESS]. [VLVWORLD]"]
["780 V-6 Coupe",1987,780,null,null,"B280F V6",null,"AW71",0,null,0,null,0,"Wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["240 DL/GL",1988,"244sedan","245wagon",null,"B230F",null,"M47",0,"AW70",0,null,0,"Early production models may use wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["440",1988,"440hatch",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["480",1988,"480coupe",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["740",1988,"740sedan","740wagon",null,"B230F",null,"M47",0,"AW70",0,null,0,"Early production models may use wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["740 Turbo",1988,"740sedan","740wagon",null,"B230FT","Garrett T3 tic",null,0,"AW71",0,null,0,"Turbo. Early production models may use wiring harness prone to deterioration, more so with the turbo because of the added heat [HARNESS]. [VLVWORLD]"]
["760 GLE",1988,"760sedan",null,null,"B280F V6",null,null,0,"AW71",0,null,0," New dashboard, flush headlights with fogs, multi-link rear end. Early production models may use wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["760 Turbo",1988,"760sedan","760wagon",null,"B230FT","Garrett T3 tic",null,0,"AW71",0,null,0,"Turbo. Smooth dashboard not prone to cracking, flush headlights with fogs, multi-link rear end in sedan. Early production models may use wiring harness prone to deterioration, more so with the turbo because of the added heat [HARNESS]. [VLVWORLD]"]
["780 Turbo Coupe",1988,780,null,null,"B230FT","Garrett T3 tic+","AW71",0,null,0,null,0,"Turbo. Multi-link rear end. Early production models may use wiring harness prone to deterioration, more so with the turbo because of the added heat [HARNESS]. [VLVWORLD]"]
["780 V-6 Coupe",1988,780,null,null,"B280F V6",null,"AW71",0,null,0,null,0," Multi-link rear end. Early production models may use wiring harness prone to deterioration [HARNESS]. [VLVWORLD]"]
["240 DL/GL",1989,"244sedan","245wagon",null,"B230F",null,"M47",0,"AW70",0,null,0,"GL not available in Canada [CARGUIDE]. [VLVWORLD]"]
["440",1989,"440hatch",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["460",1989,"460sedan",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["480",1989,"480coupe",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["740 GL",1989,"740sedan","740wagon",null,"B230F",null,"M47",0,"AW70",0,null,0,"[VLVWORLD]"]
["740 GLE",1989,"740sedan","740wagon",null,"B234F",null,"M46",0,"AW72",0,null,0,"[VLVWORLD]"]
["740 Turbo",1989,"740sedan","740wagon",null,"B230FT","Garrett T3 tic","M46",0,"AW71",0,null,0,"Tires: 195/60R-15, 0-60 in 7.8 seconds. [VLVWORLD]"]
["760 GLE",1989,"760sedan",null,null,"B280F V6",null,null,0,"AW72",0,null,0,"Smooth dashboard not prone to cracking, flush headlights with fogs, multi-link rear end in sedan. [VLVWORLD]"]
["760 Turbo",1989,"760sedan","760wagon",null,"B230FT","Garrett T3 tic",null,0,"AW72",0,null,0,"160 HP, 187 ft-lb torque. Smooth dashboard not prone to cracking, flush headlights with fogs, multi-link rear end in sedan. [VLVWORLD]"]
["780 Turbo Coupe",1989,780,null,null,"B230FT","Garrett T3 tic+","AW71",0,null,0,null,0,"Multi-link rear end. [VLVWORLD]"]
["780 V-6 Coupe",1989,780,null,null,"B280F V6",null,"AW71",0,null,0,null,0,"Multi-link rear end. [VLVWORLD]"]
["240",1990,"244sedan","245wagon",null,"B230F",null,"M47",0,"AW70",0,null,0,"[VLVWORLD]"]
["240 DL",1990,"244sedan","245wagon",null,"B230F",null,"M47",0,"AW70",0,null,0,"Same as the 240 base model but more upscale interior options. [VLVWORLD]"]
["440",1990,"440hatch",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["460",1990,"460sedan",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["480",1990,"480coupe",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["740",1990,"740sedan","740wagon",null,"B230F",null,"M47",0,"AW70",0,null,0,"European headlights, integrated front spoiler in bumper.  See <a href=\"../1990_700summary.htm\">1990 Volvo 700 Series Summary Information</a> for more information. [VLVWORLD]"]
["740 GL",1990,"740sedan","740wagon",null,"B230F",null,"M47",0,"AW70",0,null,0,"European headlights, integrated front spoiler in bumper. See <a href=\"../1990_700summary.htm\">1990 Volvo 700 Series Summary Information</a> for more information. [VLVWORLD]"]
["740 GLE",1990,"740sedan","740wagon",null,"B234F",null,"M46",0,"AW72",0,null,0,"European headlights, integrated front spoiler in bumper. See <a href=\"../1990_700summary.htm\">1990 Volvo 700 Series Summary Information</a> for more information. [VLVWORLD]"]
["740 Turbo",1990,"740sedan","740wagon",null,"B230FT","TurboG3 tic","M46",0,"AW71",0,null,0,"European headlights, integrated front spoiler in bumper. See <a href=\"../1990_700summary.htm\">1990 Volvo 700 Series Summary Information</a> for more information. [VLVWORLD]"]
["760 GLE",1990,"760sedan","760wagon",null,"B280F V6",null,"AW72",0,null,0,null,0,"Smooth dashboard not prone to cracking, flush headlights with fogs, multi-link rear end in sedan. See <a href=\"../1990_700summary.htm\">1990 Volvo 700 Series Summary Information</a> for more information. [VLVWORLD]"]
["760 Turbo",1990,"760sedan","760wagon",null,"B230FT","TurboG3 tic","AW72",0,null,0,null,0,"Smooth dashboard not prone to cracking, flush headlights with fogs, multi-link rear end in sedan. European headlights, integrated front spoiler in bumper. See <a href=\"../1990_700summary.htm\">1990 Volvo 700 Series Summary Information</a> for more information. [VLVWORLD]"]
["780 Turbo Coupe",1990,780,null,null,"B230FT","TurboG3 tic+","AW71",0,null,0,null,0,"European headlights, integrated front spoiler in bumper. See <a href=\"../1990_700summary.htm\">1990 Volvo 700 Series Summary Information</a> for more information. [VLVWORLD]"]
["780 V-6 Coupe",1990,780,null,null,"B280F V6",null,"AW71",0,null,0,null,0,"European headlights, integrated front spoiler in bumper. See <a href=\"../1990_700summary.htm\">1990 Volvo 700 Series Summary Information</a> for more information. [VLVWORLD]"]
["240 DL",1991,"244sedan","245wagon",null,"B230F",null,"M47",0,"AW70",0,null,0,"Called simply the 240 in the US, 240 DL in Canada. SE trim level for the wagon available in the US, not in Canada according to [CARGUIDE]. [VLVWORLD]"]
["440",1991,"440hatch",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["460",1991,"460sedan",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["480",1991,"480coupe",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["740",1991,"740sedan","740wagon",null,"B230F",null,"M47",0,"AW70",0,null,0,"European headlights, integrated front spoiler in bumper. [VLVWORLD]"]
["740 Turbo",1991,"740sedan","740wagon",null,"B230FT","TurboG3 tic","M46",0,"AW70",0,null,0,"European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking. [VLVWORLD]"]
["780 Turbo Coupe",1991,780,null,null,"B230FT","TurboG3 tic+","AW71",0,null,0,null,0,"Not available in Canada according to [CARGUIDE]. [VLVWORLD]"]
["940 GL",1991,"940sedan","940wagon",null,"B230F",null,null,0,"AW70",0,null,0,"European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking. [VLVWORLD]"]
["940 GLE",1991,"940sedan","940wagon",null,"B234F",null,null,0,"AW72",0,null,0,"European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking. [VLVWORLD].  Called 940 GLT in Sweden."]
["940 GLT",1991,"940sedan","940wagon",null,"B230FT","TurboG3 tic",null,0,"AW71",0,null,0,"European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking. [VLVWORLD]"]
["940 SE",1991,"940sedan","940wagon",null,"B230FT","TurboG3 tic",null,0,"AW71",0,null,0,"European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking. [VLVWORLD]"]
["940 Turbo",1991,"940sedan","940wagon",null,"B230FT","TurboG3 tic",null,0,"AW71",0,null,0,"Solid rear end.  European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking. [VLVWORLD]"]
["240 DL",1992,"244sedan","245wagon",null,"B230F",null,"M47",0,"AW70",0,null,0,"Called simply the 240 in the US, 240 DL in Canada according to [CARGUIDE]. [VLVWORLD]"]
["240 GL",1992,"244sedan",null,null,"B230F",null,"M47",0,"AW70",0,null,0,"[VLVWORLD]"]
["440",1992,"440hatch",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["460",1992,"460sedan",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["480",1992,"480coupe",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["740 GL",1992,"740sedan","740wagon",null,"B230F",null,null,0,"AW70",0,null,0,"Called simply the 740 in the US, 740 GL in Canada.  Sedan not available in Canada according to [CARGUIDE]. European headlights, integrated front spoiler in bumper. [VLVWORLD]"]
["740 Turbo",1992,"740sedan","740wagon",null,"B230FT","TurboG3 tic",null,0,"AW71",0,null,0,"European headlights, integrated front spoiler in bumper. [VLVWORLD]"]
["850 GLT (Sweden)",1992,"850sedan",null,null,"B5254S",null,"M56",0,"AW42",0,null,0,"170 HP. [EKWEBSITE]"]
["940 GL",1992,"940sedan","940wagon",null,"B230F",null,null,0,"AW70",0,null,0,"Available in the US, not available in Canada according to [CARGUIDE]. European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking. [VLVWORLD]"]
["940 GLE",1992,"940sedan","940wagon",null,"B234F",null,null,0,"AW72",0,null,0,"Available in Canada only according to [CARGUIDE]. European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking. [VLVWORLD]"]
["940 Turbo",1992,"940sedan","940wagon",null,"B230FT","TurboG3 tic",null,0,"AW71",0,null,0,"European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking. [VLVWORLD]"]
["960",1992,"960sedan","960wagon",null,"B6304F Inline 6",null,"AW30-40",0,null,0,null,0,"201 HP. European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking. [VLVWORLD]"]
[940,1993,"940sedan","940wagon",null,"B230F",null,null,0,"AW71",0,null,0,"Transmission uncertain. European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking. [VLVWORLD]"]
["240 DL/CLASSIC",1993,"244sedan","245wagon",null,"B230F",null,"M47",0,"AW70",0,null,0,"[VLVWORLD]"]
["240 GL",1993,"244sedan",null,null,"B230F",null,"M47",0,"AW70",0,null,0,"[VLVWORLD]"]
["440",1993,"440hatch",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["460",1993,"460sedan",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["480",1993,"480coupe",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["850 GLE (Sweden)",1993,"850sedan","850wagon",null,"B5252S",null,"M56",0,"AW42",0,null,0,"140 HP. [EKWEBSITE]"]
["850 GLT",1993,"850sedan","850wagon",null,"B5254S",null,"M56",0,"AW42",0,null,0,"170 HP in Sweden. 168 HP in North America. Introduced in North America this year."]
["940 GLE",1993,"940sedan","940wagon",null,"B234F",null,null,0,"AW72",0,null,0,"Available in Canada only according to [CARGUIDE]. European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking. [VLVWORLD]"]
["940 Turbo",1993,"940sedan","940wagon",null,"B230FT","TurboG3 tic",null,0,"AW71",0,null,0,"Transmission uncertain. European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking. [VLVWORLD]"]
["960",1993,"960sedan","960wagon",null,"B6304F Inline 6",null,"AW30-40",0,null,0,null,0,"European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking. [VLVWORLD]"]
[940,1994,"940sedan","940wagon",null,"B230F",null,null,0,"AW71",0,null,0,"Transmission uncertain. European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking. [VLVWORLD]"]
["440",1994,"440hatch",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["460",1994,"460sedan",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["480",1994,"480coupe",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["850 GL/SE (Sweden)",1994,"850sedan","850wagon",null,"B5254S",null,"M56",0,"AW42",0,null,0,"140 HP. [EKWEBSITE]"]
["850 Base",1994,"850sedan","850wagon",null,"B5254S",null,"M56",0,"AW42",0,null,0,"168 HP in North America.  GLT at 170 HP in Sweden [EKWEBSITE]."]
["850 Turbo",1994,"850sedan","850wagon",null,"B5234T","Turbo-Mitsu",null,0,"AW42",0,null,0,"222 HP in North America.  226 HP in Sweden [EKWEBSITE]."]
["940 Turbo",1994,"940sedan","940wagon",null,"B230FT","TurboG3 tic",null,0,"AW71",0,null,0,"Transmission uncertain. European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking. [VLVWORLD]"]
["960",1994,"960sedan","960wagon",null,"B6304F Inline 6",null,"AW30-40",0,null,0,null,0,"European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking. [VLVWORLD]"]
[940,1995,"940sedan","940wagon",null,"B230F",null,null,0,"AW71",0,null,0,"Transmission uncertain. European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking. [VLVWORLD]"]
["440",1995,"440hatch",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["460",1995,"460sedan",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["480",1995,"480coupe",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["850 Base/GLT",1995,"850sedan","850wagon",null,"B5254S",null,"M56",0,"AW42",0,null,0,"168 HP. GLT is a different trim level than the Base model. Base model not available in Canada according to [CARGUIDE].  GLT 2.5 at 170 HP in Sweden [EKWEBSITE]."]
["850 S/SE 2.0 Sweden",1995,"850sedan","850wagon",null,"B5202S",null,"M56",0,"AW42",0,null,0,"126 HP. [EKWEBSITE]"]
["850 S/SE 2.5 Sweden",1995,"850sedan","850wagon",null,"B5252S",null,"M56",0,"AW42",0,null,0,"144 HP. [EKWEBSITE]"]
["850 GLE",1995,"850sedan","850wagon",null,"B5252S",null,"M56",0,"AW42",0,null,0,"136 HP. Available in Canada, not in the US. [CARGUIDE]"]
["850 T-5R",1995,"850sedan","850wagon",null,"B5234T","Turbo-Mitsu+",null,0,"AW42",0,null,0,"240 HP.  Not available in Canada according to [CARGUIDE]."]
["850 Turbo",1995,"850sedan","850wagon",null,"B5234T","Turbo-Mitsu","M56",0,"AW42",0,null,0,"222 HP in North America.  226 HP in Sweden [EKWEBSITE]."]
["940 Turbo",1995,"940sedan","940wagon",null,"B230FT","TurboG3 tic",null,0,"AW71",0,null,0,"Transmission uncertain. European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking. [VLVWORLD]"]
["960",1995,"960sedan","960wagon",null,"B6304F Inline 6",null,"AW30-40",0,null,0,null,0,"Final drive ratio from [USWEB2]. Redesigned sheet metal - softer lines, redesigned rear suspension, colour matched roof rails on the wagon. European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking. [VLVWORLD]"]
["440",1996,"440hatch",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["460",1996,"460sedan",{"$nulls":5},0,null,0,null,0,"Small car.  Not sold in North America."]
["850 Base/GLT",1996,"850sedan","850wagon",null,"B5254S",null,"M56",0,"AW42",0,null,0,"168 HP. GLT is a different trim level than the Base model. Base model not available in Canada according to [CARGUIDE]."]
["850 S/SE 2.0 Sweden",1996,"850sedan","850wagon",null,"B5202S",null,"M56",0,"AW42",0,null,0,"126 HP. For the sedan, S trim level only. [EKWEBSITE]"]
["850 S/SE (Sweden)",1996,"850sedan","850wagon",null,"B5252S",null,"M56",0,"AW42",0,null,0,"144 HP.  For the sedan, S trim level only. [EKWEBSITE]"]
["850 GLE",1996,"850sedan","850wagon",null,"B5252S",null,"M56",0,"AW42",0,null,0,"142 HP. Available in Canada, not in the US. [CARGUIDE]"]
["850 R",1996,"850sedan","850wagon",null,"B5234T","Turbo-Mitsu+",null,0,"AW42",0,null,0,"240 HP.  Not available in Canada according to [CARGUIDE]."]
["850 Turbo",1996,"850sedan","850wagon",null,"B5234T","Turbo-Mitsu","M56",0,"AW42",0,null,0,"222 HP in North America. Also available in the Platinum Limited Edition trim.  226 HP in Sweden [EKWEBSITE]."]
["960",1996,"960sedan","960wagon",null,"B6304F2 Inline 6",null,null,0,"AW30-40",0,null,0,"Final drive ratio from [USWEB2]. Same as 1995: Redesigned sheet metal - softer lines, redesigned rear suspension, colour matched roof rails on the wagon. European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking. [VLVWORLD]"]
["S40/V40 1.8S",1996,"S40","V40",null,"B4184S",null,"manual",0,"automatic",0,null,0,"Introduced in May.  Trim name uncertain. 115 HP, 5 spd manual, 4 spd auto transmission by Aisin-Warner (Japan). Not available in North America."]
["S40/V40 1.9D",1996,"S40","V40",null,"D4192T","Turbo","manual",0,null,0,null,0,"Introduced in late 1996.  Trim name uncertain. 90 HP, 5 spd manual. Not available in North America."]
["S40/V40 2.0S",1996,"S40","V40",null,"B4204S",null,"manual",0,"automatic",0,null,0,"Introduced in May.  Trim name uncertain. 137 HP, 5 spd manual, 4 spd auto transmission by Aisin-Warner (Japan). Not available in North America."]
["850 S/SE 2.0 Sweden",1997,"850sedan","850wagon",null,"B5202S",null,"M56",0,"AW42",0,null,0,"126 HP. For the sedan, S trim level only. [EKWEBSITE]"]
["850 S/SE 2.5 Sweden",1997,"850sedan","850wagon",null,"B5252S",null,"M56",0,"AW42",0,null,0,"144 HP.  For the sedan, S trim level only. [EKWEBSITE]"]
["850 Base",1997,"850sedan","850wagon",null,"B5254S",null,"M56",0,"AW42",0,null,0,"168 HP. GLT is a different trim level than the Base model."]
["850 GLT",1997,"850sedan","850wagon",null,"B5254T","Turbo-Mitsu","M56",0,"AW42",0,null,0,"190 HP."]
["850 R (Can)",1997,"850sedan","850wagon",null,"B5234T","Turbo-Mitsu+","M56",0,"AW42",0,null,0,"247 HP for 5spd, 237HP for automatic [CAVERS]."]
["850 R (US)",1997,"850sedan","850wagon",null,"B5234T","Turbo-Mitsu+",null,0,"AW42",0,null,0,"240 HP [CAVERS]."]
["850 R (Sweden)",1997,"850sedan","850wagon",null,"B5234T","Turbo-Mitsu+",null,0,"AW42",0,null,0,"250 HP [EKWEBSITE]."]
["850 T-5",1997,"850sedan","850wagon",null,"B5234T","Turbo-Mitsu","M56",0,"AW42",0,null,0,"222 HP in North America. Also available in the Platinum Limited Edition trim.  226 HP in Sweden (called 850 Turbo) [EKWEBSITE]."]
["850 AWD (Sweden)",1997,null,"850wagon",null,"B5254T","Turbo-Mitsu","M56",0,"AW42",0,null,0,"193 HP [EKWEBSITE]. Transmissions assumed."]
["850 TDI (Sweden)",1997,"850sedan","850wagon",null,"D5252T","Turbo","M56",0,"AW42",0,null,0,"140 HP [EKWEBSITE]. Transmissions assumed."]
["960",1997,"960sedan","960wagon",null,"B6304F2 Inline 6",null,"AW30-40",0,null,0,null,0,"Final drive ratio from [USWEB2]. Same as 1995/6: Redesigned sheet metal - softer lines, redesigned rear suspension, colour matched roof rails on the wagon. European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking."]
["S40/V40 1.6S",1997,"S40","V40",null,"B4164S",null,"manual",0,null,0,null,0,"Trim name uncertain. 105 HP, 5 spd manual. Not available in North America."]
["S40/V40 1.8S",1997,"S40","V40",null,"B4184S",null,"manual",0,"automatic",0,null,0,"Trim name uncertain. 115 HP, 5 spd manual, 4 spd auto transmission by Aisin-Warner (Japan). Not available in North America."]
["S40/V40 1.9D",1997,"S40","V40",null,"D4192T","Turbo","manual",0,null,0,null,0,"Trim name uncertain. 90 HP, 5 spd manual. Not available in North America."]
["S40/V40 2.0S",1997,"S40","V40",null,"B4204S",null,"manual",0,"automatic",0,null,0,"Trim name uncertain. 137 HP, 5 spd manual, 4 spd auto transmission by Aisin-Warner (Japan). Not available in North America."]
["S40/V40 T4",1997,"S40","V40",null,"B4194T","Turbo","M56",0,null,0,null,0,"High pressure turbo, 200 HP.  Not available in North America."]
["C70 HPT",1998,"C70coupe",null,null,"B5234T","Turbo-Mitsu+","M56H",4,"AW42",2.54,null,0,"236 HP. Transmission data [VOLVO]."]
["C70 LPT",1998,null,"C70convertible",null,"B5254T","Turbo-Mitsu",null,0,"AW42",2.54,null,0,"190 HP. Transmission data [VOLVO]."]
["S40/V40 1.6S",1998,"S40","V40",null,"B4164S",null,"manual",0,null,0,null,0,"Trim name uncertain. 105 HP, 5 spd manual. Not available in North America."]
["S40/V40 1.8S",1998,"S40","V40",null,"B4184S",null,"manual",0,"automatic",0,null,0,"Trim name uncertain. 115 HP, 5 spd manual, 4 spd auto transmission by Aisin-Warner (Japan). Not available in North America."]
["S40/V40 1.9D",1998,"S40","V40",null,"D4192T","Turbo","manual",0,null,0,null,0,"Trim name uncertain. 90 HP, 5 spd manual. Not available in North America."]
["S40/V40 2.0S",1998,"S40","V40",null,"B4204S",null,"manual",0,"automatic",0,null,0,"Trim name uncertain. 137 HP, 5 spd manual, 4 spd auto transmission by Aisin-Warner (Japan). Not available in North America."]
["S40/V40 2.0T",1998,"S40","V40",null,"B4204T","Turbo","M56",0,"automatic",0,null,0,"Low pressure turbo, 160 HP.  Not available in North America."]
["S40/V40 T4",1998,"S40","V40",null,"B4194T","Turbo","M56",0,null,0,null,0,"High Pressure turbo, 200 HP.  Not available in North America."]
["S70/V70 Base",1998,"S70","V70",null,"B5254S",null,"M56",0,"AW42",0,null,0,"168 HP, Compression ratio 10.3:1"]
["S70/V70 GL (USA)",1998,"S70","V70",null,"B5254S",null,"M56",0,"AW42",0,null,0,"168 HP, Compression ratio 10.3:1"]
["S70/V70 GLT",1998,"S70","V70",null,"B5254T","Turbo-Mitsu",null,0,"AW42",0,null,0,"190 HP."]
["S70/V70 T-5",1998,"S70","V70",null,"B5234T","Turbo-Mitsu+","M56",0,"AW42",0,null,0,"236 HP."]
["S90/V90",1998,"960sedan","960wagon",null,"B6304F2 Inline 6",null,"AW30-40",0,null,0,null,0,"Final drive ratio from [USWEB2]. The S90 is a rebadged 960. Same as 1995/6/7: Redesigned sheet metal - softer lines, redesigned rear suspension, colour matched roof rails on the wagon. European headlights, integrated front spoiler in bumper, smooth dash less prone to cracking."]
["V70 AWD",1998,null,"V70",null,"B5254T","Turbo-Mitsu",null,0,"AW42",0,null,0,"190 HP."]
["V70 R AWD",1998,null,"V70",null,"B5234T","Turbo-Mitsu+",null,0,"AW42",0,null,0,"236 HP."]
["V70 XC AWD",1998,null,"V70XC",null,"B5254T","Turbo-Mitsu",null,0,"AW42",0,null,0,"190 HP."]
["C70 HPT",1999,"C70coupe","C70convertible",null,"B5234T","Turbo-Mitsu+","M56H",4,"AW42",2.54,null,0,"236 HP.  Not available in Canada according to [CARGUIDE]. Transmission data [VOLVO]."]
["C70 LPT",1999,"C70coupe","C70convertible",null,"B5254T","Turbo-Mitsu",null,0,"AW42",2.54,null,0,"190 HP. Transmission data [VOLVO]."]
["S40/V40 1.6S",1999,"S40","V40",null,"B4164S",null,"manual",0,null,0,null,0,"Trim name uncertain. 105 HP, 5 spd manual. Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 1.8 GDI",1999,"S40","V40",null,"B4184M",null,"manual",0,"automatic",0,null,0,"Trim name uncertain. 125 HP, 5 spd manual, 4 spd auto transmission by Aisin-Warner (Japan). Not available in North America."]
["S40/V40 1.8S",1999,"S40","V40",null,"B4184S",null,"manual",0,"automatic",0,null,0,"Trim name uncertain. 115 HP, 5 spd manual, 4 spd auto transmission by Aisin-Warner (Japan). Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 1.9D",1999,"S40","V40",null,"D4192T2","Turbo","manual",0,null,0,null,0,"Trim name uncertain. 95 HP, 5 spd manual. Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 2.0S",1999,"S40","V40",null,"B4204S",null,"manual",0,"automatic",0,null,0,"Trim name uncertain. 137 HP, 5 spd manual, 4 spd auto transmission by Aisin-Warner (Japan). Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 2.0T",1999,"S40","V40",null,"B4204T","Turbo","M56",0,"automatic",0,null,0,"Low pressure turbo, 160 HP.  Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 T4",1999,"S40","V40",null,"B4194T","Turbo","M56",0,null,0,null,0,"High pressure turbo, 200 HP.  Not available in North America. Info unconfirmed - assumed same as previous year."]
["S70/V70 AWD",1999,"S70","V70",null,"B5254T","Turbo-Mitsu",null,0,"AW42",0,null,0,"190 HP."]
["S70/V70 Base",1999,"S70","V70",null,"B5254S",null,"M56",0,"AW42",0,null,0,"168 HP, Compression ratio 10.3:1.  162 HP in Canada according to [CARGUIDE]."]
["S70/V70 GLT",1999,"S70","V70",null,"B5254T","Turbo-Mitsu",null,0,"AW42",0,null,0,"190 HP."]
["S70/V70 T-5",1999,"S70","V70",null,"B5234T","Turbo-Mitsu+","M56",0,"AW42",0,null,0,"236 HP."]
["S80 2.9",1999,"S80",null,null,"B6304S",null,null,0,"automatic",3.29,null,0,"201 HP [VOLVO]"]
["S80 T-6",1999,"S80",null,null,"B6284T",null,null,0,"automatic",3.29,null,0,"268 HP [VOLVO]"]
["V70 R AWD",1999,null,"V70",null,"B5234T","Turbo-Mitsu+",null,0,"AW42",0,null,0,"247 HP."]
["V70 XC AWD",1999,null,"V70XC",null,"B5254T","Turbo-Mitsu",null,0,"AW42",0,null,0,"190 HP."]
["C70 HPT",2000,"C70coupe","C70convertible",null,"B5234T","Turbo-Mitsu+","M56H",4,"AW42",2.54,null,0,"236 HP.  Transmission data [VOLVO]."]
["C70 LPT",2000,"C70coupe","C70convertible",null,"B5254T","Turbo-Mitsu",null,0,"AW42",2.54,null,0,"190 HP. Transmission data [VOLVO]."]
["S40/V40 1.6S",2000,"S40","V40",null,"B4164S",null,"manual",0,null,0,null,0,"Trim name uncertain. 105 HP, 5 spd manual. Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 1.8 GDI",2000,"S40","V40",null,"B4184M",null,"manual",0,"automatic",0,null,0,"Trim name uncertain. 125 HP, 5 spd manual, 4 spd auto transmission by Aisin-Warner (Japan). Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 1.8S",2000,"S40","V40",null,"B4184S",null,"manual",0,"automatic",0,null,0,"Trim name uncertain. 115 HP, 5 spd manual, 4 spd auto transmission by Aisin-Warner (Japan). Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 1.9D",2000,"S40","V40",null,"D4192T2","Turbo","manual",0,null,0,null,0,"Trim name uncertain. 95 HP, 5 spd manual. Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 1.9T",2000,"S40","V40",null,"B4204T","Turbo",null,0,"AW42",2.76,null,0,"FWD. Low pressure turbo, 160 HP, 4 spd auto transmission only. First year for North America.  This is the only S40/V40 model available in NA. [VOLVO]"]
["S40/V40 2.0S",2000,"S40","V40",null,"B4204S",null,"manual",0,"automatic",0,null,0,"Trim name uncertain. 137 HP, 5 spd manual, 4 spd auto transmission by Aisin-Warner (Japan). Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 2.0T",2000,"S40","V40",null,"B4204T","Turbo","M56",0,"automatic",0,null,0,"Low pressure turbo, 160 HP.  Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 T4",2000,"S40","V40",null,"B4194T","Turbo","M56",0,null,0,null,0,"High pressure turbo, 200 HP.  Not available in North America. Info unconfirmed - assumed same as previous year."]
["S70 AWD",2000,"S70",null,null,"B5244T","Turbo-Mitsu",null,0,"AW42",2.44,null,0,"190 HP."]
["S70 T-5",2000,"S70",null,null,"B5234T","Turbo-Mitsu+","M56H",4,"AW42",2.44,null,0,"236 HP. [VOLVO]. Auto tranny uncertain - 4 or 5 speed."]
["S70/V70 Base",2000,"S70","V70",null,"B5244S",null,"M56H",4,"5spd_automatic",0,null,0,"168 HP. [VOLVO]. SE trim level available in the US."]
["S70/V70 GLT",2000,"S70","V70",null,"B5244T","Turbo-Mitsu",null,0,"AW42",2.44,null,0,"190 HP. [VOLVO]. SE trim level available for the S70 GLT in the US."]
["S80 2.9",2000,"S80",null,null,"B6294S",null,null,0,"automatic",0,null,0,"197 HP"]
["S80 T-6",2000,"S80",null,null,"B6284T",null,null,0,"automatic",0,null,0,"268 HP"]
["V70 R AWD",2000,"V70",null,null,"B5244T","Turbo-Mitsu+",null,0,"AW42",2.44,null,0,"261 HP in the US, 247 HP in Canada [CARGUIDE]., 265 HP elsewhere.  5 speed auto tranny?"]
["V70 XC AWD",2000,"V70XC",null,null,"B5244T","Turbo-Mitsu",null,0,"AW42",2.65,null,0,"190 HP.  SE trim level available."]
["C70 HPT",2001,"C70coupe","C70convertible",null,"B5234T","Turbo-Mitsu+","M56H",0,"AW50-50",2.76,null,0,"236 HP.  Transmission data [VOLVO]."]
["C70 LPT",2001,null,"C70convertible",null,"B5244T","Turbo-Mitsu",null,0,"AW50-50",2.76,null,0,"190 HP. Transmission and engine data [VOLVO]."]
["S40/V40 1.6S",2001,"S40","V40",null,"B4164S",null,"manual",0,null,0,null,0,"Trim name uncertain. 105 HP, 5 spd manual. Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 1.8 GDI",2001,"S40","V40",null,"B4184M",null,"manual",0,"automatic",0,null,0,"Trim name uncertain. 125 HP, 5 spd manual, 4 spd auto transmission by Aisin-Warner (Japan). Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 1.8S",2001,"S40","V40",null,"B4184S",null,"manual",0,"automatic",0,null,0,"Trim name uncertain. 115 HP, 5 spd manual, 4 spd auto transmission by Aisin-Warner (Japan). Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 1.9D",2001,"S40","V40",null,"D4192T2","Turbo","manual",0,null,0,null,0,"Trim name uncertain. 95 HP, 5 spd manual. Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 1.9T",2001,"S40","V40",null,"B4204T","Turbo",null,0,"AW55-50",2.76,null,0,"FWD. Low pressure turbo, 162 HP, 5 spd auto transmission only. This is the only S40/V40 model available in NA.  Trim levels: 1.9T and SE  [VOLVO]"]
["S40/V40 2.0S",2001,"S40","V40",null,"B4204S",null,"manual",0,"automatic",0,null,0,"Trim name uncertain. 137 HP, 5 spd manual, 4 spd auto transmission by Aisin-Warner (Japan). Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 2.0T",2001,"S40","V40",null,"B4204T","Turbo","M56",0,"automatic",0,null,0,"Low pressure turbo, 160 HP.  Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 T4",2001,"S40","V40",null,"B4194T","Turbo","M56",0,null,0,null,0,"High pressure turbo, 200 HP.  Not available in North America. Info unconfirmed - assumed same as previous year."]
["S60 2.4",2001,"S60",null,null,"B5254S",null,"M56",0,"5spd_automatic",0,null,0,"168 HP."]
["S60 2.4T",2001,"S60",null,null,"B5254T","Turbo-Mitsu",null,0,"5spd_automatic",0,"5spd_autostick",0,"190 HP."]
["S60 T5",2001,"S60",null,null,"B5234T","Turbo-Mitsu+","M56",0,null,0,"5spd_autostick",0,"236 HP."]
["S80 2.9",2001,"S80",null,null,"B6294S",null,null,0,"automatic",0,null,0,"197 HP. [VOLVO]"]
["S80 T-6 / Exec.",2001,"S80",null,null,"B6284T",null,null,0,"automatic",0,null,0,"268 HP. [VOLVO]"]
["V70 2.4",2001,"V70rev1",null,null,"B5244S",null,"M56",4,"AW55-50",2.44,null,0,"168 HP. [VOLVO]."]
["V70 2.4T",2001,"V70rev1",null,null,"B5244T","Turbo-Mitsu",null,0,"AW55-50",2.44,"5spd_autostick",0,"190 HP. [VOLVO]"]
["V70 T5",2001,"V70rev1",null,null,"B5234T","Turbo-Mitsu+","M56",4,null,0,"5spd_autostick",0,"247 HP. [VOLVO]"]
["V70 XC",2001,"V70XCrev1",null,null,"B5244T","Turbo-Mitsu",null,0,"AW55-50",2.65,"5spd_autostick",0,"190 HP. [VOLVO]"]
["C70 HPT",2002,"C70coupe","C70convertible",null,"B5234T","Turbo-Mitsu+","M56H",0,"AW50-50",2.44,null,0,"236 HP. Transmission data [VOLVO]. AW55-50(?)"]
["C70 LPT",2002,null,"C70convertible",null,"B5244T","Turbo-Mitsu",null,0,"AW50-50",2.44,null,0,"190 HP. Transmission and engine data [VOLVO].  AW55-50(?)"]
["S40/V40 1.6S",2002,"S40","V40",null,"B4164S",null,"manual",0,null,0,null,0,"Trim name uncertain. 105 HP, 5 spd manual. Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 1.8 GDI",2002,"S40","V40",null,"B4184M",null,"manual",0,"automatic",0,null,0,"Trim name uncertain. 125 HP, 5 spd manual, 4 spd auto transmission by Aisin-Warner (Japan). Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 1.8S",2002,"S40","V40",null,"B4184S",null,"manual",0,"automatic",0,null,0,"Trim name uncertain. 115 HP, 5 spd manual, 4 spd auto transmission by Aisin-Warner (Japan). Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 1.9D",2002,"S40","V40",null,"D4192T2","Turbo","manual",0,null,0,null,0,"Trim name uncertain. 95 HP, 5 spd manual. Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 1.9T",2002,"S40","V40",null,"B4204T","Turbo",null,0,"AW55-50",2.76,null,0,"FWD. Low pressure turbo, 162 HP, 5 spd auto transmission only. This is the only S40/V40 model available in NA.  Trim levels: 1.9T and SE  [VOLVO]"]
["S40/V40 2.0S",2002,"S40","V40",null,"B4204S",null,"manual",0,"automatic",0,null,0,"Trim name uncertain. 137 HP, 5 spd manual, 4 spd auto transmission by Aisin-Warner (Japan). Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 2.0T",2002,"S40","V40",null,"B4204T","Turbo","M56",0,"automatic",0,null,0,"Low pressure turbo, 160 HP.  Not available in North America. Info unconfirmed - assumed same as previous year."]
["S40/V40 T4",2002,"S40","V40",null,"B4194T","Turbo","M56",0,null,0,null,0,"High pressure turbo, 200 HP.  Not available in North America. Info unconfirmed - assumed same as previous year."]
["S60 2.4",2002,"S60",null,null,"B5254S",null,"M56",0,"5spd_automatic",0,"5spd_autostick",0,"168 HP."]
["S60 2.4T",2002,"S60",null,null,"B5254T","Turbo-Mitsu","M56",0,"5spd_automatic",0,"5spd_autostick",0,"190 HP."]
["S60 AWD",2002,"S60",null,null,"B5254T","Turbo-Mitsu","M56",0,"5spd_automatic",0,"5spd_autostick",0,"197 HP US and Canada [CARGUIDE], 201 HP elsewhere."]
["S60 T5",2002,"S60",null,null,"B5234T","Turbo-Mitsu+","M56",0,"5spd_automatic",0,"5spd_autostick",0,"247 HP."]
["S80 2.9",2002,"S80",null,null,"B6294S",null,null,0,null,0,null,0,"194 HP (CR = 10.5:1) [VOLVO], 4 speed automatic, 4 speed 'Geartronic' automatic."]
["S80 T6",2002,"S80",null,null,"B6284T","Turbo",null,0,"automatic",0,null,0,"268 HP, 4 speed automatic, 4 speed 'Geartronic' automatic."]
["V70 2.4",2002,"V70rev1",null,null,"B5244S",null,"M56",4,"AW55-50",2.44,"5spd_autostick",0,"168 HP. [VOLVO]"]
["V70 2.4T",2002,"V70rev1",null,null,"B5244T","Turbo-Mitsu","M56",4,"AW55-50",2.44,"5spd_autostick",0,"190 HP. [VOLVO]"]
["V70 AWD",2002,"V70rev1",null,null,"B5234T","Turbo-Mitsu+","M56",4,"AW55-50",2.44,"5spd_autostick",0,"247 HP. [VOLVO]"]
["V70 T5",2002,"V70rev1",null,null,"B5234T","Turbo-Mitsu+","M56",4,"AW55-50",2.44,"5spd_autostick",0,"247 HP. [VOLVO]"]
["V70 XC AWD",2002,"V70XCrev1",null,null,"B5244T","Turbo-Mitsu","M56",4,"AW55-50",2.65,"5spd_autostick",0,"190 HP. [VOLVO]"]
["C70 HPT",2003,"C70convertible",null,null,"B5234T","Turbo-Mitsu+","M56H",0,"AW55-50",2.44,null,0,"242 HP. Transmission data [VOLVO]."]
["C70 LPT",2003,"C70convertible",null,null,"B5244T","Turbo-Mitsu",null,0,"AW55-50",2.44,null,0,"197 HP. Transmission and engine data [VOLVO]."]
["S40/V40 1.9T",2003,"S40","V40",null,"B4204T","Turbo",null,0,"AW55-50",2.44,null,0,"FWD. Low pressure turbo, 170 HP, 5 spd auto transmission only. This is the only S40/V40 model available in NA. [WHEELS]  [VOLVO]"]
["S60 2.4",2003,"S60",null,null,"B5254S",null,"M56",0,"5spd_automatic",0,null,0,"168 HP. [WHEELS] [BROCHURE]"]
["S60 2.4T",2003,"S60",null,null,"B5254T","Turbo-Mitsu",null,0,"5spd_automatic",0,"5spd_autostick",0,"197 HP. [WHEELS] [BROCHURE]"]
["S60 2.4T AWD",2003,"S60",null,null,"B5254T","Turbo-Mitsu",null,0,"5spd_automatic",0,"5spd_autostick",0,"208 HP Canada. [WHEELS] [BROCHURE]"]
["S60 T5",2003,"S60",null,null,"B5234T","Turbo-Mitsu+","M56",0,"5spd_automatic",0,"5spd_autostick",0,"247 HP. [WHEELS] [BROCHURE]"]
["S80 2.9",2003,"S80",null,null,"B6294S",null,null,0,null,0,null,0,"194 HP (CR = 10.5:1) [VOLVO], 5 speed automatic. [WHEELS] [BROCHURE]"]
["S80 T6",2003,"S80",null,null,"B6284T","Turbo",null,0,"automatic",0,null,0,"268 HP, 4 speed automatic, 4 speed 'Geartronic' automatic. [WHEELS] [BROCHURE]"]
["V70 2.4",2003,"V70rev1",null,null,"B5244S",null,"M56",4,"AW55-50",2.44,null,0,"168 HP. [WHEELS] [BROCHURE] [VOLVO]"]
["V70 2.4T",2003,"V70rev1",null,null,"B5254T","Turbo-Mitsu",null,0,"AW55-50",2.44,"5spd_autostick",0,"208 HP. [VOLVO]"]
["V70 2.4T AWD",2003,"V70rev1",null,null,"B5254T","Turbo-Mitsu+",null,0,null,0,"5spd_autostick",0,"New 2.5 litre Low Pressure turbo, 208 HP. Engine designation uncertain. [WHEELS] [BROCHURE]"]
["V70 T5",2003,"V70rev1",null,null,"B5234T","Turbo-Mitsu+","M56",4,"AW55-50",2.44,"5spd_autostick",0,"247 HP. [WHEELS] [BROCHURE] [VOLVO]"]
["V70 XC AWD",2003,"V70XCrev1",null,null,"B5254T","Turbo-Mitsu",null,0,"AW55-50",2.44,"5spd_autostick",0,"New 2.5 litre Low Pressure turbo, 208 HP. Engine designation uncertain. [WHEELS] [BROCHURE]"]
["XC90 2.5T",2003,"XC90",null,null,"B5254T","Turbo-Mitsu",null,0,"5spd_automatic",0,"5spd_autostick",0,"208 HP. Based on the S80. AWD. [WHEELS] [BROCHURE]"]
["XC90 T6",2003,"XC90",null,null,"B6284FT","Turbo",null,0,"4spd_automatic",0,null,0,"268 HP, 4 speed automatic, 4 speed 'Geartronic' automatic. Based on the S80. AWD. [WHEELS] [BROCHURE]"]
["C70 HPT",2004,"C70convertible",null,null,"B5234T","Turbo-Mitsu+","M56H",0,"AW55-50",2.44,null,0,"242 HP. Transmission data [VOLVO]."]
["C70 LPT",2004,"C70convertible",null,null,"B5244T","Turbo-Mitsu",null,0,"AW55-50",2.44,null,0,"197 HP. Transmission and engine data [VOLVO]. {WHEELS] (Canada) does not list C70 LPT Convertible in this model year."]
["S40/V40 1.9T",2004,"S40","V40",null,"B4204T","Turbo",null,0,"AW55-50",2.44,null,0,"FWD. Low pressure turbo, 170 HP, 5 spd auto transmission only. This is the only S40/V40 model available in NA. [WHEELS]  [VOLVO]"]
["S60 2.4",2004,"S60",null,null,"B5254S",null,"M56",0,"5spd_automatic",0,null,0,"168 HP. [WHEELS]"]
["S60 2.5T",2004,"S60",null,null,"B5254T","Turbo-Mitsu","M56",0,"5spd_automatic",0,"5spd_autostick",0,"208 HP. [WHEELS]"]
["S60 2.5T AWD",2004,"S60",null,null,"B5254T","Turbo-Mitsu",null,0,"5spd_automatic",0,"5spd_autostick",0,"208 HP Canada. [WHEELS]"]
["S60 R",2004,"S60",null,null,"B5254T","Turbo-Mitsu","6spd",0,"5spd_automatic",0,null,0,"300 HP. [WHEELS]"]
["S60 T5",2004,"S60",null,null,"B5234T","Turbo-Mitsu+","M56",0,"5spd_automatic",0,"5spd_autostick",0,"247 HP. [WHEELS]"]
["S80 2.9",2004,"S80",null,null,"B6294S",null,null,0,"5spd_automatic",0,null,0,"194 HP (CR = 10.5:1) [VOLVO], 4 speed automatic. [WHEELS]"]
["S80 T6",2004,"S80",null,null,"B6284T","Turbo",null,0,"automatic",0,null,0,"268 HP, 4 speed 'Geartronic' automatic. [WHEELS]"]
["V70 2.4",2004,"V70rev1",null,null,"B5244S",null,"M56",4,"AW55-50",2.44,null,0,"168 HP. [WHEELS] [VOLVO]"]
["V70 2.5T",2004,"V70rev1",null,null,"B5254T","Turbo-Mitsu",null,0,"AW55-50",2.44,"5spd_autostick",0,"208 HP. Titanium Edition also available [WHEELS] [VOLVO]"]
["V70 2.5T AWD",2004,"V70rev1",null,null,"B5254T","Turbo-Mitsu",null,0,null,0,"5spd_autostick",0,"New 2.5 litre Low Pressure turbo, 208 HP. [WHEELS] [VOLVO]"]
["V70 R",2004,"V70rev1",null,null,"B5234T","Turbo-Mitsu","6spd",0,"AW55-50",2.44,null,0,"300 HP. [WHEELS] [VOLVO]"]
["V70 T5",2004,"V70rev1",null,null,"B5234T","Turbo-Mitsu+","M56",4,null,0,null,0,"247 HP. [WHEELS] [VOLVO]"]
["XC70 (AWD)",2004,"V70XCrev1",null,null,"B5254T","Turbo-Mitsu",null,0,null,0,"AW55-50",2.65,"New 2.5 litre Low Pressure turbo, 208 HP. Engine designation uncertain. [WHEELS]"]
["XC90 2.5T",2004,"XC90",null,null,"B5254T","Turbo-Mitsu",null,0,"5spd_automatic",0,null,0,"208 HP.  AWD. 4 speed 'Geartronic' automatic.[WHEELS]"]
["XC90 T6",2004,"XC90",null,null,"B6284FT","Turbo",null,0,"4spd_automatic",0,null,0,"268 HP. AWD. [WHEELS]"]
["S40 2.4i",2005,"S40rev1",null,null,"B5244S",null,"5spd",0,"5spd_automatic",0,null,0,"FWD 168 HP, AWD available in US. [VOLVO]"]
["S40 T5",2005,"S40rev1",null,null,"B5254T","Turbo","5spd",null,"5spd_automatic",{"$nulls":3},"FWD 227 HP, AWD available in US. [VOLVO]"]
["S60 2.4",2005,"S60",null,null,"B5254S",null,"M56",0,"5spd_automatic",0,null,0,"168 HP. [VOLVO]"]
["S60 2.5T",2005,"S60",null,null,"B5254T","Turbo-Mitsu","M56",0,"5spd_automatic",0,"5spd_autostick",0,"208 HP. [VOLVO]"]
["S60 2.5T AWD",2005,"S60",null,null,"B5254T","Turbo-Mitsu",null,0,"5spd_automatic",0,"5spd_autostick",0,"208 HP. [VOLVO]"]
["S60 R",2005,"S60",null,null,"B5254T","Turbo-Mitsu","6spd",0,"5spd_automatic",0,null,0,"300 HP. [VOLVO]"]
["S60 T5",2005,"S60",null,null,"B5244T","Turbo-Mitsu+","M56",0,"5spd_automatic",0,"5spd_autostick",0,"257 HP [VOLVO]."]
["S80 2.5T",2005,"S80",null,null,"B5254T","Turbo",null,0,"automatic",0,null,0,"208 HP [VOLVO]"]
["S80 T6",2005,"S80",null,null,"B6284T","Turbo",null,0,"automatic",0,null,0,"268 HP [VOLVO]"]
["V50 2.4i",2005,"V50",null,null,"B5244S",null,"5spd",0,"5spd_automatic",0,null,0,"FWD 168 HP, AWD available in US. [VOLVO]"]
["V50 T5",2005,"V50",null,null,"B5254T","Turbo","5spd",null,"5spd_automatic",{"$nulls":3},"FWD 227 HP, AWD available in US. [VOLVO]"]
["V70 2.4",2005,"V70rev1",null,null,"B5244S",null,"M56",null,"AW55-50",{"$nulls":3},"FWD 168 HP. [VOLVO]"]
["V70 2.5T",2005,"V70rev1",null,null,"B5254T","Turbo",null,null,"AW55-50",{"$nulls":3},"FWD 208 HP. [VOLVO]"]
["V70 2.5T AWD",2005,"V70rev1",null,null,"B5254T","Turbo",null,null,"AW55-50",{"$nulls":3},"AWD 208 HP. [VOLVO]"]
["V70 R AWD",2005,"V70rev1",null,null,"B5254T","Turbo","M66",null,"TF-80SC",{"$nulls":3},"AWD 300HP. [VOLVO]"]
["V70 XC AWD",2005,"V70rev1",null,null,"B5254T","Turbo",null,null,"AW55-50",{"$nulls":3},"AWD 208 HP. [VOLVO]"]
["XC90 2.5T",2005,"XC90",null,null,"B5254T","Turbo-Mitsu",null,0,"5spd_automatic",0,null,0,"208 HP.  AWD. 4 speed 'Geartronic' automatic.[WHEELS]"]
["XC90 T6",2005,"XC90",null,null,"B6284FT","Turbo",null,0,"4spd_automatic",0,null,0,"268 HP. AWD. [WHEELS]"]
["C70",2006,"C70convertible-rev1",null,null,"B5254T","Turbo-Mitsu",{"$nulls":6},"218 HP. [VOLVO]"]
["S40 2.4i",2006,"S40rev1",null,null,"B5244S",null,"5spd",0,"5spd_automatic",0,null,0,"FWD 168 HP, AWD available in US. [VOLVO]"]
["S40 T5",2006,"S40rev1",null,null,"B5254T","Turbo","5spd",null,"5spd_automatic",{"$nulls":3},"FWD 227 HP, AWD available in US. [VOLVO]"]
["S60 2.5T",2006,"S60",null,null,"B5254T","Turbo-Mitsu","M56",0,"5spd_automatic",0,"5spd_autostick",0,"208 HP. [VOLVO]"]
["S60 2.5T AWD",2006,"S60",null,null,"B5254T","Turbo-Mitsu",null,0,"5spd_automatic",0,"5spd_autostick",0,"208 HP. [VOLVO]"]
["S60 R",2006,"S60",null,null,"B5254T","Turbo-Mitsu","6spd",0,"5spd_automatic",0,null,0,"300 HP. [VOLVO]"]
["S60 T5",2006,"S60",null,null,"B5244T","Turbo-Mitsu+","M56",0,"5spd_automatic",0,"5spd_autostick",0,"257 HP [VOLVO]."]
["S80 2.5T",2006,"S80",null,null,"B5254T","Turbo",null,0,"automatic",0,null,0,"208 HP [VOLVO]"]
["V50 2.4i",2006,"V50",null,null,"B5244S",null,"5spd",0,"5spd_automatic",0,null,0,"FWD 168 HP, AWD available in US. [VOLVO]"]
["V50 T5",2006,"V50",null,null,"B5254T","Turbo","5spd",null,"5spd_automatic",{"$nulls":3},"FWD 227 HP, AWD available in US. [VOLVO]"]
["V70 2.4",2006,"V70rev1",null,null,"B5244S",null,"M56",null,"AW55-50",{"$nulls":3},"FWD 168 HP. [VOLVO]"]
["V70 2.5T",2006,"V70rev1",null,null,"B5254T","Turbo",null,null,"AW55-50",{"$nulls":3},"FWD 208 HP. [VOLVO]"]
["V70 2.5T AWD",2006,"V70rev1",null,null,"B5254T","Turbo",null,null,"AW55-50",{"$nulls":3},"AWD 208 HP. [VOLVO]"]
["V70 R AWD",2006,"V70rev1",null,null,"B5254T","Turbo","M66",null,"TF-80SC",{"$nulls":3},"AWD 300HP. [VOLVO]"]
["V70 XC AWD",2006,"V70rev1",null,null,"B5254T","Turbo",null,null,"AW55-50",{"$nulls":3},"AWD 208 HP. [VOLVO]"]
["XC90 2.5T",2006,"XC90",null,null,"B5254T","Turbo-Mitsu",null,0,"5spd_automatic",0,null,0,"208 HP.  AWD. 4 speed 'Geartronic' automatic.[WHEELS]"]
["XC90 V8",2006,"XC90",null,null,"B8444S",null,null,0,"4spd_automatic",0,null,0,"311 HP. AWD. [VOLVO]"]
["C70",2007,"C70convertible-rev1",null,null,"B5254T","Turbo-Mitsu",{"$nulls":6},"218 HP. [VOLVO]"]
["S40 2.4i",2007,"S40rev1",null,null,"B5244S",null,"5spd",0,"5spd_automatic",0,null,0,"FWD 168 HP, AWD available in US. [VOLVO]"]
["S40 T5",2007,"S40rev1",null,null,"B5254T","Turbo","5spd",null,"5spd_automatic",{"$nulls":3},"FWD 227 HP, AWD available in US. [VOLVO]"]
["S60 2.5T",2007,"S60",null,null,"B5254T","Turbo-Mitsu","M56",0,"5spd_automatic",0,"5spd_autostick",0,"208 HP. [VOLVO]"]
["S60 2.5T AWD",2007,"S60",null,null,"B5254T","Turbo-Mitsu",null,0,"5spd_automatic",0,"5spd_autostick",0,"208 HP. [VOLVO]"]
["S60 R",2007,"S60",null,null,"B5254T","Turbo-Mitsu","6spd",0,"5spd_automatic",0,null,0,"300 HP. [VOLVO]"]
["S60 T5",2007,"S60",null,null,"B5244T","Turbo-Mitsu+","M56",0,"5spd_automatic",0,"5spd_autostick",0,"257 HP [VOLVO]."]
["S80 3.2",2007,"S80rev1",null,null,"B6324S",null,null,0,"TF-80SC",0,null,0,"235 HP.  FWD and AWD.[VOLVO]"]
["S80 V8",2007,"S80rev1",null,null,"B8444S",null,null,0,"TF-80SC",0,null,0,"268 HP. AWD. [VOLVO]"]
["V50 2.4i",2007,"V50",null,null,"B5244S",null,"5spd",0,"5spd_automatic",0,null,0,"FWD 168 HP, AWD available in US. [VOLVO]"]
["V50 T5",2007,"V50",null,null,"B5254T","Turbo","5spd",null,"5spd_automatic",{"$nulls":3},"FWD 227 HP, AWD available in US. [VOLVO]"]
["V70 2.4",2007,"V70rev1",null,null,"B5244S",null,"M56",null,"AW55-50",{"$nulls":3},"FWD 168 HP. [VOLVO]"]
["V70 2.5T",2007,"V70rev1",null,null,"B5254T","Turbo",null,null,"AW55-50",{"$nulls":3},"FWD 208 HP. [VOLVO]"]
["V70 2.5T AWD",2007,"V70rev1",null,null,"B5254T","Turbo",null,null,"AW55-50",{"$nulls":3},"AWD 208 HP. [VOLVO]"]
["V70 R AWD",2007,"V70rev1",null,null,"B5254T","Turbo","M66",null,"TF-80SC",{"$nulls":3},"AWD 300HP. [VOLVO]"]
["V70 XC AWD",2007,"V70rev1",null,null,"B5254T","Turbo",null,null,"AW55-50",{"$nulls":3},"AWD 208 HP. [VOLVO]"]
["XC90 3.2",2007,"XC90",null,null,"B6324S",null,null,0,"TF-80SC",0,null,0,"235 HP.  AWD.[VOLVO]"]
["XC90 T6",2007,"XC90",null,null,"B8444S",null,null,0,"TF-80SC",0,null,0,"268 HP. AWD. [VOLVO]"]
["C30 2.4i",2008,"C30",null,null,"B5244S",null,"5spd",0,"5spd_automatic",0,null,0,"FWD 168 HP. [VOLVO] Transmissions uncertain."]
["C30 T5",2008,"C30",null,null,"B5254T","Turbo","5spd",null,"5spd_automatic",{"$nulls":3},"FWD 227 HP. [VOLVO] Transmissions uncertain."]
["C70",2008,"C70convertible-rev1",null,null,"B5254T","Turbo-Mitsu",{"$nulls":6},"227 HP. [VOLVO]"]
["S40 2.4i",2008,"S40rev1",null,null,"B5244S",null,"5spd",0,"5spd_automatic",0,null,0,"FWD 168 HP, AWD available in US. [VOLVO]"]
["S40 T5",2008,"S40rev1",null,null,"B5254T","Turbo","5spd",null,"5spd_automatic",{"$nulls":3},"FWD 227 HP, AWD available in US. [VOLVO]"]
["S60 2.5T",2008,"S60",null,null,"B5254T","Turbo-Mitsu","M56",0,"5spd_automatic",0,"5spd_autostick",0,"208 HP. [VOLVO]"]
["S60 2.5T AWD",2008,"S60",null,null,"B5254T","Turbo-Mitsu",null,0,"5spd_automatic",0,"5spd_autostick",0,"208 HP. [VOLVO]"]
["S60 T5",2008,"S60",null,null,"B5244T","Turbo-Mitsu+","M56",0,"5spd_automatic",0,"5spd_autostick",0,"257 HP [VOLVO]."]
["S80 3.0T",2008,"S80rev1",null,null,"B6304T","Turbo",null,null,"TF-80SC",{"$nulls":3},"281 HP. AWD [VOLVO]"]
["S80 3.2",2008,"S80rev1",null,null,"B6324S",null,null,0,"TF-80SC",0,null,0,"235 HP.  FWD and AWD [VOLVO]"]
["S80 V8",2008,"S80rev1",null,null,"B8444S",null,null,0,"TF-80SC",0,null,0,"311 HP. AWD. [VOLVO]"]
["V50 2.4i",2008,"V50",null,null,"B5244S",null,"5spd",0,"5spd_automatic",0,null,0,"FWD 168 HP, AWD available in US. [VOLVO]"]
["V50 T5",2008,"V50",null,null,"B5254T","Turbo","5spd",null,"5spd_automatic",{"$nulls":3},"FWD 227 HP, AWD available in US. [VOLVO]"]
["V70 3.0T",2008,"V70rev2",null,null,"B6304T","Turbo",null,null,"TF-80SC",{"$nulls":3},"FWD 281 HP [VOLVO]"]
["V70 3.2",2008,"V70rev2",null,null,"B6324S",{"$nulls":3},"TF-80SC",{"$nulls":3},"FWD 235 HP [VOLVO]"]
["XC70 3.0T",2008,"V70rev2",null,null,"B6304T","Turbo",null,null,"TF-80SC",{"$nulls":3},"AWD 281 HP [VOLVO]"]
["XC70 3.2",2008,"V70rev2",null,null,"B6324S",{"$nulls":3},"TF-80SC",{"$nulls":3},"AWD 235 HP [VOLVO]"]
["XC90 3.2",2008,"XC90",null,null,"B6324S",null,null,0,"TF-80SC",0,null,0,"235 HP.  AWD.[VOLVO]"]
["XC90 T6",2008,"XC90",null,null,"B8444S",null,null,0,"TF-80SC",0,null,0,"268 HP. AWD. [VOLVO]"]
["C30 2.4i",2009,"C30",null,null,"B5244S",null,"5spd",0,"5spd_automatic",0,null,0,"FWD 168 HP. [VOLVO] Transmissions uncertain."]
["C30 T5",2009,"C30",null,null,"B5254T","Turbo","5spd",null,"5spd_automatic",{"$nulls":3},"FWD 227 HP. [VOLVO] Transmissions uncertain."]
["C70",2009,"C70convertible-rev1",null,null,"B5254T","Turbo-Mitsu",{"$nulls":6},"227 HP. [VOLVO]"]
["S40 2.4i",2009,"S40rev1",null,null,"B5244S",null,"5spd",0,"5spd_automatic",0,null,0,"FWD 168 HP, AWD available in US. [VOLVO]"]
["S40 T5",2009,"S40rev1",null,null,"B5254T","Turbo","5spd",null,"5spd_automatic",{"$nulls":3},"FWD 227 HP, AWD available in US. [VOLVO]"]
["S60 2.5T",2009,"S60",null,null,"B5254T","Turbo-Mitsu","M56",0,"5spd_automatic",0,"5spd_autostick",0,"208 HP. [VOLVO]"]
["S60 2.5T AWD",2009,"S60",null,null,"B5254T","Turbo-Mitsu",null,0,"5spd_automatic",0,"5spd_autostick",0,"208 HP. [VOLVO]"]
["S60 T5",2009,"S60",null,null,"B5244T","Turbo-Mitsu+","M56",0,"5spd_automatic",0,"5spd_autostick",0,"257 HP [VOLVO]."]
["S80 3.0T",2009,"S80rev1",null,null,"B6304T","Turbo",null,null,"TF-80SC",{"$nulls":3},"281 HP. AWD [VOLVO]"]
["S80 3.2",2009,"S80rev1",null,null,"B6324S",null,null,0,"TF-80SC",0,null,0,"235 HP.  [VOLVO]"]
["S80 V8",2009,"S80rev1",null,null,"B8444S",null,null,0,"TF-80SC",0,null,0,"311 HP. AWD. [VOLVO]"]
["V50 2.4i",2009,"V50",null,null,"B5244S",null,"5spd",0,"5spd_automatic",0,null,0,"FWD 168 HP, AWD available in US. [VOLVO]"]
["V50 T5",2009,"V50",null,null,"B5254T","Turbo","5spd",null,"5spd_automatic",{"$nulls":3},"FWD 227 HP, AWD available in US. [VOLVO]"]
["V70 3.0T",2009,"V70rev2",null,null,"B6304T","Turbo",null,null,"TF-80SC",{"$nulls":3},"FWD 281 HP [VOLVO]"]
["V70 3.2",2009,"V70rev2",null,null,"B6324S",{"$nulls":3},"TF-80SC",{"$nulls":3},"FWD 235 HP [VOLVO]"]
["XC70 3.0T",2009,"V70rev2",null,null,"B6304T","Turbo",null,null,"TF-80SC",{"$nulls":3},"AWD 281 HP [VOLVO]"]
["XC70 3.2",2009,"V70rev2",null,null,"B6324S",{"$nulls":3},"TF-80SC",{"$nulls":3},"AWD 235 HP [VOLVO]"]
["XC90 3.2",2009,"XC90",null,null,"B6324S",null,null,0,"TF-80SC",0,null,0,"235 HP.  AWD.[VOLVO]"]
["XC90 T6",2009,"XC90",null,null,"B8444S",null,null,0,"TF-80SC",0,null,0,"268 HP. AWD. [VOLVO]"]
["C30 2.4i",2010,"C30",null,null,"B5244S",null,"5spd",0,"5spd_automatic",0,null,0,"FWD 168 HP.  This model Not available in North America. [VOLVO] Transmissions uncertain."]
["C30 T5",2010,"C30",null,null,"B5254T","Turbo","5spd",null,"5spd_automatic",{"$nulls":3},"FWD 227 HP. [VOLVO] Transmissions uncertain."]
["C70",2010,"C70convertible-rev1",null,null,"B5254T","Turbo-Mitsu",{"$nulls":6},"227 HP. [VOLVO]"]
["S40 2.4i",2010,"S40rev1",null,null,"B5244S",null,"5spd",0,"5spd_automatic",0,null,0,"FWD 168 HP, AWD available in US. [VOLVO]"]
["S40 T5",2010,"S40rev1",null,null,"B5254T","Turbo","5spd",null,"5spd_automatic",{"$nulls":3},"FWD 227 HP, AWD available in US. [VOLVO]"]
["S80 3.0T",2010,"S80rev1",null,null,"B6304T","Turbo",null,null,"TF-80SC",{"$nulls":3},"281 HP. AWD [VOLVO]"]
["S80 3.2",2010,"S80rev1",null,null,"B6324S",null,null,0,"TF-80SC",0,null,0,"235 HP.  [VOLVO]"]
["S80 V8",2010,"S80rev1",null,null,"B8444S",null,null,0,"TF-80SC",0,null,0,"311 HP. AWD. [VOLVO]"]
["V50 2.4i",2010,"V50",null,null,"B5244S",null,"5spd",0,"5spd_automatic",0,null,0,"FWD 168 HP, AWD available in US. [VOLVO]"]
["V50 T5",2010,"V50",null,null,"B5254T","Turbo","5spd",null,"5spd_automatic",{"$nulls":3},"FWD 227 HP, AWD available in US. [VOLVO]"]
["V70 3.0T",2010,"V70rev2",null,null,"B6304T","Turbo",null,null,"TF-80SC",{"$nulls":3},"FWD 281 HP [VOLVO]"]
["V70 3.2",2010,"V70rev2",null,null,"B6324S",{"$nulls":3},"TF-80SC",{"$nulls":3},"FWD 235 HP [VOLVO]"]
["XC60 3.2",2010,"XC60",null,null,"B6324S",{"$nulls":3},"TF-80SC",{"$nulls":3},"FWD/AWD 235 HP."]
["XC60 T6 AWD",2010,"XC60",null,null,"B6304T","Turbo",null,null,"TF-80SC",{"$nulls":3},"AWD 281 HP."]
["XC70 3.0T",2010,"V70rev2",null,null,"B6304T","Turbo",null,null,"TF-80SC",{"$nulls":3},"AWD 300 HP [VOLVO]"]
["XC70 3.2",2010,"V70rev2",null,null,"B6324S",{"$nulls":3},"TF-80SC",{"$nulls":3},"AWD 240 HP [VOLVO]"]
["XC90 3.2",2010,"XC90",null,null,"B6324S",null,null,0,"TF-80SC",0,null,0,"235 HP.  AWD.[VOLVO]"]
["XC90 T6",2010,"XC90",null,null,"B8444S",null,null,0,"TF-80SC",0,null,0,"268 HP. AWD. [VOLVO]"]
["C30 2.4i",2011,"C30",null,null,"B5244S",null,"5spd",0,"5spd_automatic",0,null,0,"FWD 168 HP.  This model Not available in North America. [VOLVO] Transmissions uncertain."]
["C30 T5",2011,"C30",null,null,"B5254T","Turbo","5spd",null,"5spd_automatic",{"$nulls":3},"FWD 227 HP. [VOLVO] Transmissions uncertain."]
["C60 R-Design",2011,"S60rev1",null,null,"B6304T","Turbo",null,null,"TF-80SC",{"$nulls":3},"AWD 325 HP. "]
["C60 T5",2011,"S60rev1",null,null,"B5244T","Turbo-Mitsu+","M56",0,"5spd_automatic",0,"5spd_autostick",0,"FWD 250 HP [VOLVO]."]
["C60 T6",2011,"S60rev1",null,null,"B6304T","Turbo",null,null,"TF-80SC",{"$nulls":3},"AWD 300 HP."]
["C70",2011,"C70convertible-rev1",null,null,"B5254T","Turbo-Mitsu",{"$nulls":6},"227 HP. [VOLVO]"]
["S40 T5",2011,"S40rev1",null,null,"B5254T","Turbo","5spd",null,"5spd_automatic",{"$nulls":3},"FWD 227 HP. [VOLVO]"]
["S80 3.2",2011,"S80rev1",null,null,"B6324S",null,null,0,"TF-80SC",0,null,0,"FWD 240 HP.  [VOLVO]"]
["S80 T6 AWD",2011,"S80rev1",null,null,"B6304T","Turbo",null,null,"TF-80SC",{"$nulls":3},"AWD 300 HP. AWD [VOLVO]"]
["V50 T5",2011,"V50",null,null,"B5254T","Turbo","5spd",null,"5spd_automatic",{"$nulls":3},"FWD 227 HP. [VOLVO]"]
["XC60 3.2",2011,"XC60",null,null,"B6324S",{"$nulls":3},"TF-80SC",{"$nulls":3},"FWD/AWD 240 HP."]
["XC60 R-Design",2011,"XC60",null,null,"B6304T","Turbo",null,null,"TF-80SC",{"$nulls":3},"AWD 325 HP. "]
["XC60 T6 AWD",2011,"XC60",null,null,"B6304T","Turbo",null,null,"TF-80SC",{"$nulls":3},"AWD 300 HP."]
["XC70 3.0T",2011,"V70rev2",null,null,"B6304T","Turbo",null,null,"TF-80SC",{"$nulls":3},"AWD 300 HP [VOLVO].  Not available in Canada."]
["XC70 3.2",2011,"V70rev2",null,null,"B6324S",{"$nulls":3},"TF-80SC",{"$nulls":3},"FWD/AWD 240 HP [VOLVO]. AWD only in Canada."]
["XC90 3.2",2011,"XC90",null,null,"B6324S",null,null,0,"TF-80SC",0,null,0,"FWD/AWD 240 HP. [VOLVO].  AWD only in Canada."]
["C30 T5",2012,"C30",null,null,"B5254T","Turbo","5spd",null,"5spd_automatic",{"$nulls":3},"FWD 227 HP. [VOLVO] Transmissions uncertain."]
["C70",2012,"C70convertible-rev1",null,null,"B5254T","Turbo-Mitsu",{"$nulls":6},"227 HP. [VOLVO]"]
["S60 T5",2012,"S60rev1",null,null,"B5254T","Turbo",null,null,"TF-80SC",{"$nulls":3},"AWD 247 HP. [VOLVO]"]
["S60 T6 AWD",2012,"S60rev1",null,null,"B6304T","Turbo",null,null,"TF-80SC",{"$nulls":3},"AWD 300 HP. [VOLVO]"]
["S60 T6 AWD",2012,"S60rev1",null,null,"B6304T","Turbo",null,null,"TF-80SC",{"$nulls":3},"AWD 300 HP. [VOLVO]"]
["XC60 3.2",2012,"XC60",null,null,"B6324S",{"$nulls":3},"TF-80SC",{"$nulls":3},"FWD/AWD 240 HP."]
["XC60 T6 AWD",2012,"XC60",null,null,"B6304T","Turbo",null,null,"TF-80SC",{"$nulls":3},"AWD 300 HP."]
["XC70 3.0T",2012,"V70rev2",null,null,"B6304T","Turbo",null,null,"TF-80SC",{"$nulls":3},"AWD 300 HP [VOLVO]."]
["XC70 3.2",2012,"V70rev2",null,null,"B6324S",{"$nulls":3},"TF-80SC",{"$nulls":3},"FWD/AWD 240 HP [VOLVO]."]
["XC90 3.2",2012,"XC90",null,null,"B6324S",null,null,0,"TF-80SC",0,null,0,"FWD/AWD 235 HP. [VOLVO]."]
["XC90 V8",2012,"XC90",null,null,"B8444S",{"$nulls":3},"TF-80SC",{"$nulls":3},"AWD 311 Hp. [VOLVO]"]

{"sheet":"chassis","index":2,"n_rows":105,"n_cols":12,"rows_kept":105}
["Volvo Chassis Page",{"$nulls":10},"S40/V40/V50/C30 series"]
[{"$f":"COUNTA(A4:A1006)","v":102}]
["name","family","#doors","wb","len","width","height","wt","turn rad","front suspension","rear suspension","notes"]
["OV4open","Early series",4,112.2,1,1,1,1,1,null,null,"Open car. [LINDH]"]
["OV4pickup","Early series",2,112.2,1,1,1,1,1,null,null,"Pickup body. [LINDH]"]
["OV4frame","Early series",0,112.2,1,1,1,1,1,null,null,"Presumably a 'frame only' version. [LINDH]"]
["PV4sedan","Early series",4,112.2,1,1,1,1,1,null,null,"[LINDH]"]
["PV4frame","Early series",0,112.2,1,1,1,1,1,null,null,"'Frame only' version. [LINDH]"]
["PV650frame","Early series",0,116.1,1,1,1,1,1,null,null,"'Frame only' version. [LINDH]"]
["PV650special","Early series",0,139.8,1,1,1,1,1,null,null,"'Frame only' ambulance and hearse version. [LINDH]"]
["PV651sedan","Early series",4,116.1,1,1,1,1,1,null,null,"Mechanical braking system. [LINDH]"]
["PV652sedan","Early series",4,116.1,1,1,1,1,1,null,null,"Hydraulic braking system. [LINDH]"]
["PV653sedan","Early series",4,116.1,1,1,1,1,1,null,null,"Based on the PV652sedan chassis but with an all-metal body. [LINDH]"]
["PV655frame","Early series",0,116.1,1,1,1,1,1,null,null,"'Frame only' version. Basis for the PV653/4 sedans. [LINDH]"]
["PV656frame","Early series",0,116.1,1,1,1,1,1,null,null,"'Frame only' version. Basis for the PV658/9 sedans. [LINDH]"]
["PV657frame","Early series",0,139.8,1,1,1,1,1,null,null,"'Frame only' ambulance version. [LINDH]"]
["PV658sedan","Early series",4,116.1,1,1,1,1,1,null,null,"[LINDH]"]
["PV36sedan","Early series",4,116.1,1,1,1,1,1,null,null,"New 'American-like' sleek steel body on frame. [LINDH]"]
["PV51sedan","Early series",4,113.4,1,1,1,1,1,null,null,"Based on the PV36. Steel body on frame. [LINDH]"]
["PV51frame","Early series",0,113.4,1,1,1,1,1,null,null,"'Frame only' version. 86 HP. [LINDH]"]
["PV53sedan","Early series",4,113.4,1,1,1,1,1,null,null,"Base version. 86 HP.  Spare tire in boot lid. [LINDH]"]
["PV54sedan","Early series",4,113.4,1,1,1,1,1,null,null,"Base version. 86 HP.  Spare tire in enlarged boot. [LINDH]"]
["PV56frame","Early series",0,113.4,1,1,1,1,1,null,null,"'Frame only' version. 50 HP ECG engine. [LINDH]"]
["PV60sedan","Early series",4,112.2,1,1,1,1,1,null,null,"90 HP. [LINDH]"]
["PV61frame","Early series",0,112.2,1,1,1,1,1,null,null,"90 HP. [LINDH]"]
["TR670frame","Early series",0,122,1,1,1,1,1,null,null,"'Frame only' version. [LINDH]"]
["TR671taxi","Early series",4,122,1,1,1,1,1,null,null,"Taxi version. [LINDH]"]
["TR677frame","Early series",0,128,1,1,1,1,1,null,null,"'Frame only' version. [LINDH]"]
["TR678taxi","Early series",4,128,1,1,1,1,1,null,null,"Taxi version. [LINDH]"]
["PV801taxi","Early series",4,128,1,1,1,1,1,null,null,"Taxi version, with partition. [LINDH]"]
["PV802taxi","Early series",4,128,1,1,1,1,1,null,null,"Taxi version, without partition. [LINDH]"]
["PV800frame","Early series",0,128,1,1,1,1,1,null,null,"'Frame only' version. [LINDH]"]
["PV810frame","Early series",0,139.8,1,1,1,1,1,null,null,"Long wheelbase 'Frame only' version. [LINDH]"]
["PV821taxi","Early series",4,128,1,1,1,1,1,null,null,"Taxi version, with partition. [LINDH]"]
["PV822taxi","Early series",4,128,1,1,1,1,1,null,null,"Taxi version, without partition. [LINDH]"]
["PV825frame","Early series",0,128,1,1,1,1,1,null,null,"'Frame only' version. [LINDH]"]
["PV831taxi","Early series",4,128,1,1,1,1,1,null,null,"Taxi version, with partition. [LINDH]"]
["PV832taxi","Early series",4,128,1,1,1,1,1,null,null,"Taxi version, without partition. [LINDH]"]
["PV835frame","Early series",0,128,1,1,1,1,1,null,null,"'Frame only' version. [LINDH]"]
["444sedan","PV series",2,1,1,1,1,1,1,null,"solid axle","Unit body construction, split windshield made of 2 flat glass sections. [VLVWORLD]"]
["445wagon","PV series",3,1,1,1,1,1,1,null,"solid axle","Body on frame construction, split windshield made of 2 flat glass sections, frame also used to produce pickup trucks and vans. [VLVWORLD]"]
["445pickup","PV series",3,1,1,1,1,1,1,null,"solid axle","Body on frame construction, split windshield made of 2 flat glass sections, frame also used to produce wagons and vans. [VLVWORLD]"]
["445van","PV series",3,1,1,1,1,1,1,null,"solid axle","Body on frame construction, split windshield made of 2 flat glass sections, frame also used to produce wagons and pickups. [VLVWORLD]"]
["544sedan","PV series",2,1,1,1,1,1,29.9,null,"solid axle","Unit body construction, single piece windshield. [VLVWORLD],[UKCLUB1]"]
["210wagon","PV series",3,1,1,1,1,1,1,null,"solid axle","This is a wagon version of the 544, body on frame construction. [VLVWORLD]"]
["P1900","PV series",2,94.5,1,1,1,1,1,null,null,"Convertible sports car."]
["1800coupe","P1800 series",2,96.5,171,67,50.4,2529,31,null,null,"[VLVWORLD],[UKCLUB1]"]
["1800wagon","P1800 series",3,1,1,1,1,1,31.5,null,null,"[VLVWORLD],[UKCLUB1]"]
["120sedan","120 series",4,102.5,175,65.7,59.2,2360,34,"independent coil with sway bar","solid axle","Data based on 1968 2 door model.  Front disc  and rear drum brakes. [VLVWORLD],[UKCLUB1]"]
["130sedan","120 series",2,102.5,175,65.7,59.2,2360,34,"independent coil with sway bar","solid axle","This is the 2 door version of the 120sedan body.  Data based on 1968 2 door model. Front disc  and rear drum brakes. [VLVWORLD],[UKCLUB1]"]
["220wagon","120 series",5,102.5,176.5,63.8,60.2,2640,34,"independent coil","solid axle with progressive auxiliary springs","This is the 4 door wagon version of the 120sedan. [VLVWORLD],[UKCLUB1],[USWEB1]"]
["142sedan","140/160 series",2,102.4,182.7,68.1,56.7,2520,30.2,null,"solid axle","Data based on 1968 2 door model.  Disc brakes front and rear. [VLVWORLD],[UKCLUB1]"]
["144sedan","140/160 series",4,102.4,182.7,68.1,56.7,2600,30.2,null,"solid axle","Data based on 1968 4 door model.  Disc brakes front and rear. [VLVWORLD],[UKCLUB1]"]
["145wagon","140/160 series",5,102.4,182.7,68.1,56.7,2870,30.2,null,"solid axle","Data based on 1968 wagon model.  Disc brakes front and rear. [VLVWORLD],[UKCLUB1]"]
["164sedan","140/160 series",4,1,1,1,1,1,31.6,null,null,"[VLVWORLD],[UKCLUB1]"]
["242sedan","240/260 series",2,104.3,189.9,67.3,56.3,2919,32.5,"MacPherson strut","solid axle","[VLVWORLD],[UKCLUB1]"]
["244sedan","240/260 series",4,104.3,189.9,67.3,56.3,2919,32.5,"MacPherson strut","solid axle","[VLVWORLD],[UKCLUB1]"]
["245wagon","240/260 series",5,104.3,190.7,67.3,57.5,3051,32.5,"MacPherson strut","solid axle","[VLVWORLD],[UKCLUB1]"]
["262sedan","240/260 series",2,1,1,1,1,1,32.5,null,null,"[VLVWORLD],[UKCLUB1]"]
["262coupe","240/260 series",2,1,1,1,1,1,32.5,null,null,"Lowered roof. [VLVWORLD],[UKCLUB1]"]
["264sedan","240/260 series",4,1,1,1,1,1,32.5,null,null,"[VLVWORLD],[UKCLUB1]"]
["265wagon","240/260 series",5,1,1,1,1,1,32.5,null,null,"[VLVWORLD],[UKCLUB1]"]
["66sedan","300 series",2,89,1,1,1,1,1,null,null,"Small car, DAF origins.  Poor quality."]
["66combi","300 series",3,89,1,1,1,1,1,null,null,"Small car, DAF origins.  Poor quality."]
["343hatch","300 series",3,94.5,1,1,1,1,30.2,null,null,"[UKCLUB1]"]
["345wagon","300 series",5,94.5,1,1,1,1,30.2,null,null,"[UKCLUB1]"]
["360hatch","300 series",3,94.5,1,1,1,1,30.7,null,null,"[UKCLUB1]"]
["360sedan","300 series",4,94.5,1,1,1,1,30.7,null,null,"[UKCLUB1]"]
["360wagon","300 series",5,94.5,1,1,1,1,30.7,null,null,"[UKCLUB1]"]
["440hatch","400 series",5,100,176,68,1,2960,1,null,null,"Hatchback"]
["460sedan","400 series",4,100,176,68,1,2960,1,null,null,"4 dr. sedan.  Dimensions uncertain."]
["480coupe","400 series",2,100,176,68,1,2960,1,null,null,"2 dr. Coupe"]
["740sedan","700/900 series",4,109.1,188.4,68.9,55.5,2954,32,"MacPherson strut","solid axle","Base chassis. [VLVWORLD]"]
["740wagon","700/900 series",5,109.1,188.4,68.9,56.5,3082,32,"MacPherson strut","solid axle","Aluminum tailgate to save weight. [VLVWORLD]"]
["760sedan","700/900 series",4,109.1,188.4,68.9,55.5,3272,32,"MacPherson strut","independent, self-leveling","[VLVWORLD]"]
["760wagon","700/900 series",5,109.1,188.4,68.9,56.5,3272,32,"MacPherson strut","solid axle, self-leveling","Aluminum tailgate to save weight. [VLVWORLD]"]
["780_nonIRS","700/900 series",2,109.1,188.7,68.9,55.1,3415,32.5,"MacPherson strut","solid axle, self-leveling","[VLVWORLD]"]
["780","700/900 series",2,109.1,188.7,68.9,55.1,3415,32.5,"MacPherson strut","independent, self-leveling","[VLVWORLD]"]
["940sedan","700/900 series",4,109.1,188.4,68.9,55.5,3272,32,"MacPherson strut","independent, self-leveling","[VLVWORLD]"]
["940wagon","700/900 series",5,109.1,188.4,68.9,56.5,3272,32,"MacPherson strut","independent, self-leveling","Aluminum tailgate to save weight. [VLVWORLD]"]
["960sedan","700/900 series",4,109.1,191.7,69.3,55.5,3515,32,"MacPherson strut","independent, self-leveling","[VLVWORLD]"]
["960wagon","700/900 series",5,109.1,191.7,69.3,55.5,3515,32,"MacPherson strut","independent, self-leveling","Aluminum tailgate to save weight, numerical data based on sedan."]
["850sedan","850/S70/V70 series",4,104.9,183.5,69.3,55.1,3140,33.5,"MacPherson strut",null,"[UKCLUB1]"]
["850wagon","850/S70/V70 series",5,104.9,183.5,69.3,55.1,3140,33.5,"MacPherson strut",null,"Dimensions and weight approximate. [UKCLUB1]"]
["S70","850/S70/V70 series",4,104.9,185.8,69.3,55.1,3148,33.5,"MacPherson strut",null,"The S70 is the successor to the 850 sedan. [UKCLUB1]"]
["C70coupe","850/S70/V70 series",2,104.7,186,71.1,55.1,3325,33.5,"MacPherson strut",null,"Coupe derived from the S70. [UKCLUB1].  Dimensions and weight [VOLVO] (1998 specs)"]
["C70convertible","850/S70/V70 series",2,104.7,185.7,71.7,56.3,3630,38.4,"MacPherson strut",null,"[UKCLUB1] [WHEELS]. Dimensions and weight [VOLVO] (1998 specs)"]
["C70convertible-rev1","850/S70/V70 series",2,103.9,175.9,69.7,57.2,3805,34.9,"MacPherson strut",null,"[VOLVO] (Owner's Manual 2006)"]
["V70","850/S70/V70 series",5,108.5,185.5,71,58.7,3368,-1,"MacPherson strut",null,"The V70 is the successor to the 850 wagon"]
["V70XC","850/S70/V70 series",5,109,0,0,0,0,-1,"MacPherson strut",null,"The V70XC is the 'Cross Country' version of the V70 with added ground clearance and styling cues."]
["V70rev1","850/S70/V70 series",5,109,186,73,58.7,3368,39,"MacPherson strut",null,"The V70 is the successor to the 850 wagon.  In 2001, the chassis dimensions were revised."]
["V70XCrev1","850/S70/V70 series",5,109,186.3,73.2,61.5,3593.5,39,"MacPherson strut",null,"The V70XC is the 'Cross Country' version of the V70 with added ground clearance and styling cues.  Dimensions taken from [WHEELS] March, 2003. Wheelbase assumed same as V70. In 2001, the chassis dimensions were revised."]
["V70rev2","850/S70/V70 series",5,110.9,189.9,73.3,60.9,3860,35.8,"MacPherson strut",null,"The V70 is the successor to the 850 wagon.  In 2008 model year (North America), the chassis dimensions were revised.  It might have appeared in 2007 in Europe.  Turning radius in the V70R is 43.3 ft. [VOLVO]"]
["V70XCrev2","850/S70/V70 series",5,110.8,190.5,73.3,63.1,4155,null,"MacPherson strut",null,"The V70XC is the 'Cross Country' version of the V70 with added ground clearance and styling cues. [VOLVO]"]
["S60","850/S70/V70 series",4,107,180.2,71,56.2,3500,35.4,"MacPherson strut",null,"The S60 is the successor to the S70 sedan. AWD weighs 1502 kg. Dimensions taken from [WHEELS] March, 2003. Turning radius 35.4 to 38.7 [VOLVO]."]
["S60rev1","850/S70/V70 series",4,109.3,182.2,73.4,58.4,3548,37.1,"MacPherson strut",null,"Turning Rradius 39 ft for 6 cylinder engines [VOLVO]."]
["XC60","850/S70/V70 series",null,109.2,182.2,62.4,67.4,null,null,"MacPherson strut",null,"[VOLVO] (Owner's Manual 2010)"]
["S40","S40/V40 series",4,101,178.8,67.6,56,2976,36.7,null,null,"4 dr. sedan. Dimensions taken from [WHEELS] March, 2003. [VOLVO]"]
["V40","S40/V40 series",5,101,178.8,67.6,56.1,3020,36.7,null,null,"Wagon.  Dimensions taken from [WHEELS] March, 2003. [VOLVO]"]
["S40rev1","S40/V40 series",4,103.9,175.9,69.7,57.2,3165,34.9,null,null,"4 dr. sedan. [VOLVO]"]
["V50","S40/V40 series",5,103.9,177.7,69.7,57.2,3220,34.9,null,null,"Wagon. [VOLVO]"]
["C30","S40/V40 series",3,103.9,167.4,70.2,57,3155,null,"MacPherson strut",null,"Smaller, sportier 3-door version of the S40, based on the S40rev1 chassis. [VOLVO]"]
["S80","S80 series",4,109.9,189.8,72.1,57.2,3583,39,"MacPherson strut",null,"FWD replacement for the RWD 960sedan/S90. Large turning circle.  Dimensions taken from [VOLVO] spec sheet 2004."]
["S80rev1","S80 series",4,111.6,191,73.3,58.8,3725,36.7,"MacPherson strut",null,"Turning radius 36.7-40 ft. [VOLVO].  Dimensions taken from [VOLVO] 2007."]
["XC90","SUV series",5,112.5,188.9,74.4,68.9,4510.7,39,"MacPherson strut",null,"SUV, based on the S80.  Dimensions taken from [WHEELS] March, 2003. Also [VOLVO]."]

{"sheet":"engine","index":3,"n_rows":64,"n_cols":9,"rows_kept":64}
["Volvo Engine Page"]
[{"$f":"COUNTA(A4:A1010)","v":61}]
["name "," #cyl "," #valves "," disp "," compression "," fuel type "," fuel delivery "," turbo "," Notes"]
["DA",4,2,1.94,4.9,"gasoline","Solex carb","no","Side valve inline 4, 3 main bearings. [LINDH]"]
["DB",6,2,3.01,5.1,"gasoline","Solex or Nife carb","no","Side valve inline 6, 7 main bearings. [LINDH]"]
["EB",6,2,3.266,-1,"gasoline","Carb","no","Based on the DB engine. [LINDH]"]
["EC",6,2,3.67,6.1,"gasoline","Carb","no","Based on the EB engine. [LINDH]"]
["ECG",6,2,3.67,6.1,"gasoline","Carb","no","Producer gas version of the EC engine, 50 HP, used during the war, mainly by the military. [LINDH]"]
["ED",6,2,3.67,6.5,"gasoline","Carb","no","Higher output EC engine. [LINDH]"]
["B4B",4,2,1.414,-1,"gasoline","Carb (Carter 1947-53, Zenith 1954-55)","no","OHV inline 4, a simple cast iron 3-main bearing engine introduced in 1944.  [VOLUPARTS] for fuel delivery info."]
["B14A",4,2,1.414,9.5,"gasoline","Dual carb (SU H2)","no","[URBANCIC], [GRIMSHAW1]. [VOLUPARTS] for fuel delivery info."]
["B16A",4,2,1.583,8.2,"gasoline","Carb","no","OHV inline 4, the B16 was introduced in 1956, first of the 'red blocks'. [GRIMSHAW1], [CLARKE70]"]
["B16B",4,2,1.583,8.2,"gasoline","Dual carb (Skinner's Union H4)","no","OHV inline 4, the B16 was introduced in 1956, first of the 'red blocks'. [GRIMSHAW1], [CLARKE70]"]
["B18A",4,2,1.778,8.7,"gasoline","Carb (SU or ZS175CD)","no","OHV inline 4, the B18 was introduced in 1960, first 5-main bearing engine. [URBANCIC], [GRIMSHAW1]"]
["B18B",4,2,1.778,10,"gasoline","Dual Carb (Skinner's Union HS 6 or ZS175CD)","no","OHV inline 4, the B18 was introduced in 1960, first 5-main bearing engine. [URBANCIC], [GRIMSHAW1]"]
["B18D",4,2,1.778,8.7,"gasoline","Dual carb (SU-HS6 or ZS175CD)","no","OHV inline 4, introduced in 1960, first 5-main bearing engine, high compression. [URBANCIC], [GRIMSHAW1], [USWEB1]"]
["B18E",4,2,1.721,-1,"gasoline","Carb","no","Renault block modified for Volvo for FWD 400 series. [GRIMSHAW1]"]
["B19",4,2,1.986,-1,"gasoline",null,null,"OVC, introduced in 1976 as an underbored version of the B21 [GRIMSHAW1]. The B19 is mentioned in [GRIMSHAW1] as the engine for the 340/360 series, so this is assumed for all years."]
["B20A",4,2,1.986,8.7,"gasoline","Single Carb (ZS175CD2SE or SU HIF6)","no","OHV inline 4, the B20 was introduced in 1968. [URBANCIC], [GRIMSHAW1]"]
["B20B",4,2,1.986,9.5,"gasoline","Dual Carb (ZS175CD for 1968-71 or SU H1F6 for 1971-74)","no","OHV inline 4, the B20 was introduced in 1968. [URBANCIC], [GRIMSHAW1]. [VOLUPARTS] for fuel delivery id and compression ratio (CR=9.5 for 1969-70, 9.3 in 1971, 8.7 for 1972-74)."]
["B20E",4,2,1.986,10.5,"gasoline","Bosch D-Jetronic","no","OHV inline 4, the B20 was introduced in 1968. [URBANCIC], [GRIMSHAW1]. [VOLUPARTS] for fuel delivery id and compression ratio."]
["B20F",4,2,1.986,8.7,"gasoline","Bosch D-Jetronic (1972-73), Bosch K-Jetronic (1974-75)","no","OHV inline 4, the B20 was introduced in 1968.  [URBANCIC], [GRIMSHAW1]. [VOLUPARTS] for fuel delivery id and compression ratio."]
["B21A",4,2,2.127,7.5,"gasoline","Single Carb (Skinner's Union HIF6 for 1981 or Zenith Stromberg 175CD2SE otherwise)","no","OHC inline 4, first OVC with alloy cross-flow cylinder head. [URBANCIC], [GRIMSHAW1]. [VOLUPARTS] for fuel delivery id, also CR =8.5 for 1975-81 and 9.3 for 1982-84."]
["B21F",4,2,2.127,9.3,"gasoline","Bosch K-Jetronic high pressure continuous fuel injection for 1976-82, Bosch LH 1.0 for 1982","no","OHC inline 4, first OVC with alloy cross-flow cylinder head. [URBANCIC], [GRIMSHAW1]. [VOLUPARTS] for fuel delivery id and compression ratio."]
["B21FT",4,2,2.127,7.5,"gasoline","Bosch K-Jetronic high pressure continuous fuel injection","yes","OHC inline 4, first OVC with alloy cross-flow cylinder head. [URBANCIC], [GRIMSHAW1]"]
["B21FTi",4,2,2.127,7.5,"gasoline","Bosch K-Jetronic high pressure continuous fuel injection","yes","OHC inline 4, first OVC with alloy cross-flow cylinder head. Same as B21FT but with intercooled turbo. [GRIMSHAW1]"]
["B23E",4,2,2.316,10,"gasoline","Bosch K-Jetronic high pressure continuous fuel injection","no","Overhead cam, low friction, tough and durable, non-interference head [URBANCIC], [GRIMSHAW1]"]
["B23F",4,2,2.316,10,"gasoline","Bosch LH 2.0-Jetronic pulsed fuel injection","no","Overhead cam, low friction, tough and durable, non-interference head [URBANCIC], [GRIMSHAW1].. [VOLUPARTS] for fuel delivery id, says compression ratio = 10.3."]
["B23FT",4,2,2.316,8.7,"gasoline","Bosch LH 2.0-Jetronic pulsed fuel injection","yes","Overhead cam, tough and durable, non-interference head [URBANCIC]. Forged crank, rods and pistons [MICHAEL1].. [VOLUPARTS] for fuel delivery id."]
["B230F",4,2,2.316,10,"gasoline","Bosch LH 2.2-Jetronic pulsed fuel injection for 1985-88, LH 2.4 for 1989-93, LH 3.1 for 1991-93","no","Overhead cam, low friction, tough and durable, non-interference head. [URBANCIC], [GRIMSHAW1]. [VOLUPARTS] for fuel delivery id."]
["B234F",4,4,2.316,10,"gasoline","Bosch LH 2.4-Jetronic pulsed fuel injection","no","Double overhead cam (DOHC), low friction, tough and durable, interference head so make sure to change the timing belt every 50,000 miles! [URBANCIC], [GRIMSHAW1]"]
["B230FT",4,2,2.316,8.7,"gasoline","Bosch LH 2.2-Jetronic pulsed fuel injection for 1985-89","yes","Overhead cam, low friction, tough and durable, non-interference head. [URBANCIC], [GRIMSHAW1].  \"The '90-on models ... had better flowing manifolds. The piston cooling started in '93. Cast crank. From '85 to about '89, the B230FT had smaller 9mm con rods. From around '89 to '95, the B230FT has larger 13mm con rods.  The latest blocks were the strongest ('95 being the best).\" [MICHAEL1].. [VOLUPARTS] for fuel delivery id."]
["B30A",6,2,2.978,9.3,"gasoline","Dual Carb (Zenith Stromberg 175CD2SE)","no","OHV Inline 6 cylinder. [GRIMSHAW1]. [VOLUPARTS] for fuel delivery id and compression ratio.  CR=8.7 for USA."]
["B30E",6,2,2.978,10,"gasoline","Bosch D-Jetronic","no","OHV Inline 6 cylinder. [URBANCIC], [GRIMSHAW1]. [VOLUPARTS] for fuel delivery id and compression ratio."]
["B30F",6,2,2.978,8.7,"gasoline","Bosch D-Jetronic","no","OHV Inline 6 cylinder, USA version? [URBANCIC], [GRIMSHAW1]. [VOLUPARTS] for fuel delivery id and compression ratio."]
["B27F V6",6,2,2.644,-1,"gasoline","fuel injection","no","PVR engine, apparently prone to numerous problems. See <a href=\"../volvohome.htm#PVR\">Common Problems</a> for more information. [URBANCIC], [GRIMSHAW1]"]
["B28F V6",6,2,2.849,9.5,"gasoline","fuel injection","no","PVR engine, improved B27F but still prone to numerous problems.  See <a href=\"../volvohome.htm#PVR\">Common Problems</a> for more information. [URBANCIC], [GRIMSHAW1]"]
["B280F V6",6,2,2.849,9.5,"gasoline","fuel injection","no","low friction, PVR engine, apparently prone to numerous problems.  See <a href=\"../volvohome.htm#PVR\">Common Problems</a> for more information. [URBANCIC], [GRIMSHAW1]"]
["B4164S",4,4,1.6,-1,"gasoline","fuel injection","no","DOHC Inline 4-cylinder. [GRIMSHAW1]"]
["B4184S",4,4,1.731,-1,"gasoline","fuel injection","no","DOHC Inline 4-cylinder. [URBANCIC], [GRIMSHAW1]"]
["B4184M",4,4,1.731,-1,"gasoline","fuel injection","no","DOHC Inline 4-cylinder.  Extreme lean-burn engine from Mitsubishi. [URBANCIC], [GRIMSHAW1]"]
["B4204S",4,4,1.948,-1,"gasoline","fuel injection","no","DOHC Inline 4-cylinder. [URBANCIC], [GRIMSHAW1]"]
["B4204T",4,4,1.948,9,"gasoline","fuel injection","yes","DOHC Inline 4-cylinder. [URBANCIC] [VOLVO]"]
["B4194T",4,4,1.948,10.3,"gasoline","fuel injection","yes","DOHC Inline 4-cylinder, reduced bore, turbo variant of the B4202F. [URBANCIC], [GRIMSHAW1]"]
["B5234T",5,4,2.319,8.5,"gasoline","fuel injection","yes","DOHC Inline 5-cylinder. [URBANCIC], [GRIMSHAW1]"]
["B5244S",5,4,2.44,10.3,"gasoline","fuel injection","no","DOHC Inline 5-cylinder. [VOLVO]"]
["B5244T",5,4,2.44,9,"gasoline","fuel injection","yes","DOHC Inline 5-cylinder. [VOLVO]"]
["B5202S",5,2,2,-1,"gasoline","fuel injection","no","Specs unknown, available in Sweden at least [EKWEBSITE]."]
["B5252S",5,2,2.435,10.1,"gasoline","Fenix 5.2 fuel injection","no","DOHC Inline 5-cylinder. May have been available in other years than indicated. [URBANCIC], [GRIMSHAW1], [VLVWORLD].  CR 10.3 in Sweden [EKWEBSITE]."]
["B5254S",5,4,2.435,10.5,"gasoline","Bosch Motronic sequential fuel injection","no","DOHC Inline 5-cylinder. [URBANCIC], [GRIMSHAW1]"]
["B5254T",5,4,2.435,9,"gasoline","Bosch Motronic sequential fuel injection","yes","DOHC Inline 5-cylinder. [URBANCIC], [GRIMSHAW1]"]
["B6304F Inline 6",6,4,2.922,10,"gasoline","Bosch Motronic sequential fuel injection","no","DOHC, low friction, possible porous block problem causing coolant leakage.  See <a href=\"../volvohome.htm#POROUS\">Common Problems</a> for more information. [URBANCIC], [GRIMSHAW1]"]
["B6304F2 Inline 6",6,4,2.922,10,"gasoline","fuel injection","no","DOHC, low friction. [GRIMSHAW1]"]
["B6284FT",6,4,2.8,8.7,"gasoline","fuel injection","yes","DOHC Inline 6-cylinder, twin turbo, based on the B6304F2, variable valve timing. [URBANCIC], [GRIMSHAW1]"]
["B6284T",6,4,2.78,8.5,"gasoline","fuel injection","yes","[VOLVO] based on specs from 1999 S80."]
["B6294S",6,4,2.92,10.7,"gasoline","fuel injection","no","[VOLVO] based on specs from 2000 S80."]
["B6304S",6,4,2.92,10.7,"gasoline","fuel injection","no","[VOLVO] based on specs from 1999 S80."]
["B6304T",6,4,2.95,9.3,"gasoline","fuel injection","yes","[VOLVO] Transverse inline 6, turbo."]
["B6324S",6,4,3.19,10.8,"gasoline","fuel injection","no","[VOLVO] Transverse inline 6, non-turbo."]
["B8444S",8,4,4.41,10.4,"gasoline","fuel injection","no","[VOLVO]"]
["D24T",6,2,2.383,-1,"diesel","fuel injection","yes","[URBANCIC], [GRIMSHAW1]"]
["D4192T",4,2,1.87,-1,"diesel","fuel injection","yes","[URBANCIC]"]
["D4192T2",4,2,1.87,-1,"diesel","fuel injection","yes","[URBANCIC]"]
["D5252T",5,2,2.435,-1,"diesel","fuel injection","yes","[URBANCIC]  Displacement assumed."]

{"sheet":"tranny","index":4,"n_rows":39,"n_cols":12,"rows_kept":39}
["Volvo Tranny Page"]
[{"$f":"COUNTA(A4:A1008)","v":35}]
["name "," type "," maker "," #gears "," r1 "," r2 "," r3 "," r4 "," r5 "," r6 "," r7 "," Notes"]
["H6","manual","Koping Engineering, AB Volvo",3,-1,-1,-1,-1,-1,-1,-1,"Synchromesh on 2nd and 3rd. [GRIMSHAW96]"]
["M3","manual","Koping Engineering, AB Volvo",3,-1,-1,-1,-1,-1,-1,-1,"3 speed?"]
["M4","manual","Koping Engineering, AB Volvo",4,-1,-1,-1,-1,-1,-1,-1,"Fully synchronized. [GRIMSHAW96]"]
["M30","manual","Koping Engineering, AB Volvo",3,-1,-1,-1,-1,-1,-1,-1,"Fully synchronized, same as M40 but with 1st gear blanked out. [GRIMSHAW96]"]
["M31","manual","Koping Engineering, AB Volvo",4,-1,-1,-1,-1,-1,-1,-1,"3 speed + electric o/d, Fully synchronized, same as M31 with electric overdrive. [GRIMSHAW96]"]
["M40","manual","Koping Engineering, AB Volvo",4,3.13,1.99,1.36,1,-1,-1,-1,"Fully synchronized. [GRIMSHAW96],[USWEB1], [CLARKE70]"]
["M41","manual","Koping Engineering, AB Volvo",5,3.13,1.99,1.36,1,0.77,-1,-1,"Fully synchronized, M40 with electric overdrive. [GRIMSHAW96], [CLARKE70]"]
["M400","manual","Koping Engineering, AB Volvo",4,-1,-1,-1,-1,-1,-1,-1,"Fully synchronized, heavy duty version of the M40. [GRIMSHAW96]"]
["M410","manual","Koping Engineering, AB Volvo",5,-1,-1,-1,-1,-1,-1,-1,"Fully synchronized, M400 with electric overdrive. [GRIMSHAW96]"]
["M45","manual","Koping Engineering, AB Volvo",4,-1,-1,-1,-1,-1,-1,-1,"Fully synchronized. [GRIMSHAW96]"]
["M46","manual","Koping Engineering, AB Volvo",5,4.03,2.16,1.37,1,0.79,-1,-1,"4 speed + electric o/d, Fully synchronized, used for higher torque engines. [GRIMSHAW96], [GRIMSHAW99]"]
["M47","manual","Koping Engineering, AB Volvo",5,4.03,2.16,1.37,1,0.82,-1,-1,"Fully synchronized, apparently not as strong as the M46. Road&Track in 1989 says OD is 0.80. [GRIMSHAW96], [GRIMSHAW99]"]
["M55","manual","Koping Engineering, AB Volvo",5,-1,-1,-1,-1,-1,-1,-1,"Fully synchronized, transaxle for FWD pre-production 850s [GRIMSHAW96]"]
["M56","manual","Koping Engineering, AB Volvo",5,3.38,1.9,1.19,0.87,0.7,-1,-1,"Fully synchronized, transaxle for FWD. [GRIMSHAW96], [GRIMSHAW99] [VOLVO]"]
["M56H","manual","Koping Engineering, AB Volvo",5,3.07,1.77,1.19,0.87,0.7,-1,-1,"Fully synchronized, transaxle for FWD. Higher 1st and 2nd gears [VOLVO]"]
["M66","manual",null,6,{"$nulls":7},"[VOLVO]"]
["5spd","manual",{"$nulls":9},"Manual transmission of unknown specifications."]
["6spd","manual",null,6,-1,-1,-1,-1,-1,-1,-1,"Fully synchronized, transaxle for FWD. "]
["manual","manual",null,3,-1,-1,-1,-1,-1,-1,-1,"Manual transmission of unknown specifications."]
["BW35","automatic","Borg & Warner (USA)",3,2.39,1.45,1,-1,-1,-1,-1,"[GRIMSHAW96]"]
["BW55","automatic","Borg & Warner (USA)",3,-1,-1,-1,-1,-1,-1,-1,"[GRIMSHAW96]"]
["AW55","automatic","Aisin-Warner (Japan)",3,-1,-1,-1,-1,-1,-1,-1,"Same as the BW55 but produced under licence. [GRIMSHAW96]"]
["AW50-50","automatic","Aisin-Warner (Japan)",5,4.77,2.1,1.96,1.32,1.02,null,null,"From 2000 C70 US Owner's Manual [VOLVO]"]
["AW55-50","automatic","Aisin-Warner (Japan)",5,4.77,3,1.96,1.32,1.02,null,null,"From 2001-2004 S40 US Owner's Manual [VOLVO]"]
["AW42","automatic","Aisin-Warner (Japan)",4,3.61,2.06,1.37,0.98,-1,-1,-1,"Transaxle for FWD, with overdrive and lockup torque converter. [GRIMSHAW96], [GRIMSHAW99] [VOLVO]"]
["AW70","automatic","Aisin-Warner (Japan)",4,2.45,1.45,1,0.69,-1,-1,-1,"With overdrive (AW70), or with overdrive and lockup torque converter (AW70L). [GRIMSHAW96], [GRIMSHAW99].  US turbo models did not have lockup but European turbo models did. [BRICKBOARD-FAQ]"]
[]
["AW71","automatic","Aisin-Warner (Japan)",4,2.45,1.45,1,0.69,-1,-1,-1,"With overdrive (AW71), or with overdrive and lockup torque converter (AW71L). [GRIMSHAW96], [GRIMSHAW99].  US turbo models did not have lockup but European turbo models did. [BRICKBOARD-FAQ]"]
["AW72","automatic","Aisin-Warner (Japan)",4,2.83,1.49,1,0.73,-1,-1,-1,"with overdrive and lockup torque converter, reinforced casting. [GRIMSHAW96], [GRIMSHAW99]"]
["AW30-40","automatic","Aisin-Warner (Japan)",4,2.8,1.53,1,0.71,-1,-1,-1,"with overdrive and lockup torque converter. [GRIMSHAW96], [GRIMSHAW99]"]
["ZF-4HP22L","automatic","Zahnradfabrik-Friedrichshafen (Germany)",4,2.48,1.48,1,0.73,-1,-1,-1,"lockup torque converter coming in at about 57 mph. [GRIMSHAW96], [GRIMSHAW99]"]
["TF-80SC","automatic","Aisin-Warner (Japan)",6,4.148,2.37,1.556,1.155,0.8591,0.686,null,"Also called the AWTF-80 SC , AWF21, AF40-6, AM6 and AW6A-EL.[WIKI-1]"]
["4spd_automatic","automatic",null,4,-1,-1,-1,-1,-1,-1,-1,"4 speed automatic transmission of unknown specifications."]
["5spd_automatic","automatic",null,5,-1,-1,-1,-1,-1,-1,-1,"5 speed automatic transmission of unknown specifications used in the S70/V70."]
["5spd_autostick","automatic",null,5,-1,-1,-1,-1,-1,-1,-1,"5 speed automatic transmission with 'manual mode' of unknown specifications used in the S70/V70."]
["automatic","automatic",null,3,-1,-1,-1,-1,-1,-1,-1,"Automatic transmission of unknown specifications."]

{"sheet":"turbos","index":5,"n_rows":12,"n_cols":2,"rows_kept":12}
["Volvo Turbo Page"]
[{"$f":"COUNTA(A4:A1000)","v":9}]
["Turbo name","Notes"]
["Turbo","Specifics unknown."]
["Turbo_i","Intercooled, specifics unknown."]
["Garrett T3 turbo","Large turbo causing a 'turbo lag'."]
["Garrett T3 tic","Large turbo causing a 'turbo lag'.  Intercooled."]
["Garrett T3 tic+","Large turbo causing a 'turbo lag'.  Higher boost at specified rpm."]
["TurboG3 tic","Generation 3: smaller turbo giving faster spoolup and less 'turbo lag'. Either a Garrett T25 or a Mitsubishi TD04.  Intercooled."]
["TurboG3 tic+","Generation 3 + higher boost,  smaller turbo giving faster spoolup and less 'turbo lag.' Either a Garrett T25 or a Mitsubishi TD04.  Intercooled."]
["Turbo-Mitsu","Mitsubishi at 9.6psi, intercooled."]
["Turbo-Mitsu+","Mitsubishi at 10 psi, intercooled."]

{"sheet":"sources","index":6,"n_rows":25,"n_cols":2,"rows_kept":25}
["Volvo Source Page"]
[{"$f":"COUNTA(A4:A1004)","v":22}]
["Source ID","Notes"]
["[BROCHURE]","Volvo official brochure."]
["[BRICKBOARD-FAQ]","See the FAQ at <a href=\"http://www.brickboard.com\" target=\"_blank\">http://wwwbrickboard.com</a>."]
["[BRYANT]","Email from Tom Bryant, 2004.12.15."]
["[CLARKE70]","R.M. Clarke, <i>Volvo 120 Series, 1956-1970</i>, Brookland Books, England, circa 1970, ISBN 0 907073 16 6."]
["[CAVERS]","Email from Glen Cavers, 2004.02.15"]
["[CARGUIDE]","CAR GUIDE, published yearly giving brief model description and price of Canadian models."]
["[EKWEBSITE]","<a href=\"http://www.swipnet.se/E_K/\" target=\"_blank\">http://www.swipnet.se/E_K/</a>. EK's Car Site listing models in Sweden as of 2002-01-10.  Unfortunately, the site appears to be no longer available."]
["[GRIMSHAW1]","<a href=\"http://www3.telus.net/Volvo_Books/specart11.html\" target=\"_blank\">http://www3.telus.net/Volvo_Books/specart11.html</a> and <a href=\"http://www3.telus.net/Volvo_Books/specart5.html\" target=\"_blank\">http://www3.telus.net/Volvo_Books/specart5.html</a>. Articles by Paul Grimshaw on Volvo Engines."]
["[GRIMSHAW96]","Paul Grimshaw, <i>The Gothenburg Bible, A Guide to Long-Term, Cost-Efficient & Worry-Free Volvo Ownership</i>,  ZOD Publishing, 2nd edition 1996.  Order information at <a href=\"http://www3.telus.net/Volvo_Books/home.html\" target=\"_blank\">http://www3.telus.net/Volvo_Books/home.html</a>."]
["[GRIMSHAW99]","Paul Grimshaw, <i>The Volvo Performance Handbook</i>,  ZOD Publishing, 2nd edition 1999.  Order information at <a href=\"http://www3.telus.net/Volvo_Books/home.html\" target=\"_blank\">http://www3.telus.net/Volvo_Books/home.html</a>."]
["[HARNESS]","Wiring harnesses for 1983 to 1987 (and possibly early 1988) Volvo cars tend to crack and deteriorate prematurely, more so with the turbo because of the added heat. See <a href=\"../volvohome.htm#HARNESS\">Common Problems</a> for more information."]
["[LINDH]","Bjorn-Eric Lindh, <i>VOLVO, The Cars - From the 20s to the 80s</i>, ISBN 91-86442-08-2, Forlagshuset Norden AB, 1984.  A revision for the 90s is available."]
["[MICHAEL1]","Email posted on <a href=\"http://www.brickboard.com\" target=\"_blank\">The BrickBoard</a> by Michael ?, 2002.02.04."]
["[UKCLUB1]","<a href=\"http://www.volvoclub.org.uk/turn_circles.htm\" target=\"_blank\">www.volvoclub.org.uk/turn_circles.htm</a>, UK Volvo club page on turning circles.  Data extracted 2002.05.07."]
["[URBANCIC]","<a href=\"http://www2.mf.uni-lj.si/~jurbancic/engines.htm\" target=\"_blank\">http://www2.mf.uni-lj.si/~jurbancic/engines.htm</a>. This web site by J. Urbancic contains lots of good info on Volvo engines. Data extracted 2002.02.20."]
["[USWEB1]","<a href=\"http://new.volvocars.com\" target=\"_blank\">http://new.volvocars.com</a>. Useful set of model pages on the official US Volvo site. You have to log on as a US resident to the Owner's Library. Data extracted 2002.05.05."]
["[USWEB2]","<a href=\"http://new.volvocars.com\" target=\"_blank\">http://new.volvocars.com</a>. Useful set of model pages on the official US Volvo site. You have to log on as a US resident to the Owner's Library. Data extracted 2006.11.06 (Thanks to Al Sichelstiel for the reference.)"]
["[VLVWORLD]","<a href=\"http://www.vlvworld.com\" target=\"_blank\">www.vlvworld.com</a>, parts supplier.  This web site contains lots of good info on parts, production figures, engine designations and specs, colour codes, and VIN numbers.  Data extracted 2002.01.12."]
["[VOLUPARTS]","<a href=\"http://www.mindspring.com/~voluparts/engines.htm\" target=\"_blank\">http://www.mindspring.com/~voluparts/engines.htm</a>.  Voluparts, parts supplier.  This web page contains lots of engine information for engines from 1947 to 1991, including tune-up specs.  For some reason, there is no link to this data page from their main site at <a href=\"http://www.voluparts.com/index.html\" target=\"_blank\">http://www.voluparts.com/index.html</a>."]
["[VOLVO]","Volvo US website - Owner's Manuals at <a href=\"http://www.volvocars.com/us/top/yourvolvo/volvo-vehicle-information-library/pages/default.aspx\" target=\"_blank\">http://www.volvocars.com/us/top/yourvolvo/volvo-vehicle-information-library/pages/default.aspx</a>"]
["[WHEELS]","World of Wheels, published yearly giving brief model description and price of Canadian models. Web site: <a href=\"http://www.wheels.ca\" target=\"_blank\">www.wheels.ca</a>. "]
["[WIKI-1]","<a href\"http://en.wikipedia.org/wiki/AWTF-80_SC\"target=\"_blank\">http://en.wikipedia.org/wiki/AWTF-80_SC</a> Wikipedia info extracted 2012.12.16.  "]